A B C D E F G H I J K L M N O P Q R S T U V W

## A

ACTION_DOWN - Static variable in class com.datecs.universalreader.TouchEvent
  A pressed gesture has started, the touch event contains a valid location of event.
ACTION_UP - Static variable in class com.datecs.universalreader.TouchEvent
  A pressed gesture has finished, the touch event does not contains a valid location.
AES - Class in com.datecs.crypto
  Helper methods to encrypt or decrypt with AES algorithm.
AES() - Constructor for class com.datecs.crypto.AES
afi - Variable in class com.datecs.rfid.ContactlessCard
  The card AFI (Available for ISO15 cards only).
ALIGN_CENTER - Static variable in class com.datecs.printer.Printer
  The printing object is centered.
ALIGN_LEFT - Static variable in class com.datecs.printer.Printer
  The printing object is left aligned.
ALIGN_RIGHT - Static variable in class com.datecs.printer.Printer
  The printing object is left aligned.
alignKey(byte[]) - Static method in class com.datecs.crypto.TripleDES
  Convert from 16 bytes double length Triple DES to full size 24 bytes key.
AnsiIso - Class in com.datecs.biometric
  Finger Image-Based Data Interchange Format parser.
AnswerToReset - Class in com.datecs.smartcard
  This class represents the smart card response ATR as defined in ISO/IEC 7816-4.
AnswerToReset(byte[]) - Constructor for class com.datecs.smartcard.AnswerToReset
  Constructs a new instance of this class from a given byte array.
anticollision() - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Returns the serial number of one of requested Mifare cards.
atqa - Variable in class com.datecs.rfid.ContactlessCard
  The card ATQA (Available for MIFARE cards only).
authenticate(char, int, byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Authenticate mifare card block with direct key data.
authenticate(char, int, int) - Method in class com.datecs.rfid.ISO14443Card
  Authenticate mifare card block with previously stored key.
authenticate(int, int, int, byte[]) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Authenticates Mifare card for operation.
authenticate(int, int, int, int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Authenticates Mifare card for operation with key stored into Mifare reader EEPROM memory.
authenticateAES(byte[], int) - Method in class com.datecs.rfid.ISO14443Card.DESFire

## B

Barcode - Class in com.datecs.barcode
  This class represents an extracted barcode information.
BARCODE_ALL - Static variable in class com.datecs.barcode.Barcode
  ALL (Not specify)
BARCODE_AZTEK - Static variable in class com.datecs.barcode.Barcode
  AZTEK
BARCODE_CCA - Static variable in class com.datecs.barcode.Barcode
  CCA
BARCODE_CCB - Static variable in class com.datecs.barcode.Barcode
  CCB
BARCODE_CCC - Static variable in class com.datecs.barcode.Barcode
  CCC
BARCODE_CODABAR - Static variable in class com.datecs.barcode.Barcode
  CODABAR
BARCODE_CODABAR - Static variable in class com.datecs.printer.Printer
  CODABAR (NW-7) barcode type.
BARCODE_CODABAR_ABC - Static variable in class com.datecs.barcode.Barcode
  CODABAR ABC
BARCODE_CODABAR_CX - Static variable in class com.datecs.barcode.Barcode
  CODABAR CX
BARCODE_CODE11 - Static variable in class com.datecs.barcode.Barcode
  CODE11
BARCODE_CODE128 - Static variable in class com.datecs.barcode.Barcode
  CODE128
BARCODE_CODE128 - Static variable in class com.datecs.printer.Printer
  CODE 128 barcode type.
BARCODE_CODE128AUTO - Static variable in class com.datecs.printer.Printer
  CODE 128 Auto barcode type.
BARCODE_CODE25_I2OF5 - Static variable in class com.datecs.barcode.Barcode
  CODE25 I2OF5
BARCODE_CODE25_NI2OF5 - Static variable in class com.datecs.barcode.Barcode
  CODE25 NI2OF5
BARCODE_CODE39 - Static variable in class com.datecs.barcode.Barcode
  CODE39
BARCODE_CODE39 - Static variable in class com.datecs.printer.Printer
  CODE 39 barcode type.
BARCODE_CODE39_FULL - Static variable in class com.datecs.barcode.Barcode
  CODE39 FULL
BARCODE_CODE93 - Static variable in class com.datecs.barcode.Barcode
  CODE93
BARCODE_CODE93 - Static variable in class com.datecs.printer.Printer
  CODE 93 barcode type.
BARCODE_CPCBINARY - Static variable in class com.datecs.barcode.Barcode
  CPCBINARY
BARCODE_DATAMATRIX - Static variable in class com.datecs.barcode.Barcode
  DATAMATRIX
BARCODE_DUN14 - Static variable in class com.datecs.barcode.Barcode
  DUN14
BARCODE_EAN128 - Static variable in class com.datecs.barcode.Barcode
  EAN128
BARCODE_EAN128 - Static variable in class com.datecs.printer.Printer
  EAN 128 barcode type.
BARCODE_EAN13 - Static variable in class com.datecs.barcode.Barcode
  EAN13
BARCODE_EAN13 - Static variable in class com.datecs.printer.Printer
  EAN13 (JAN13) barcode type.
BARCODE_EAN13_2 - Static variable in class com.datecs.barcode.Barcode
  EAN13 2
BARCODE_EAN13_5 - Static variable in class com.datecs.barcode.Barcode
  EAN13 5
BARCODE_EAN2 - Static variable in class com.datecs.barcode.Barcode
  EAN2
BARCODE_EAN5 - Static variable in class com.datecs.barcode.Barcode
  EAN5
BARCODE_EAN8 - Static variable in class com.datecs.barcode.Barcode
  EAN8
BARCODE_EAN8 - Static variable in class com.datecs.printer.Printer
  EAN 8 (JAN8) barcode type.
BARCODE_EAN8_2 - Static variable in class com.datecs.barcode.Barcode
  EAN8 2
BARCODE_EAN8_5 - Static variable in class com.datecs.barcode.Barcode
  EAN8 5
BARCODE_GS1DATABAR - Static variable in class com.datecs.barcode.Barcode
  GS1 DATABAR
BARCODE_IATA - Static variable in class com.datecs.barcode.Barcode
  IATA
BARCODE_INTELLIGENT_MAIL - Static variable in class com.datecs.barcode.Barcode
  INTELLIGENT_MAI
BARCODE_ITA_PHARMA - Static variable in class com.datecs.barcode.Barcode
  ITA PHARMA
BARCODE_ITF - Static variable in class com.datecs.printer.Printer
  ITF barcode type.
BARCODE_ITF14 - Static variable in class com.datecs.barcode.Barcode
  ITF14
BARCODE_KOREAN_POSTAL - Static variable in class com.datecs.barcode.Barcode
  KOREAN POSTAL
BARCODE_LAST - Static variable in class com.datecs.barcode.Barcode
  LAST
BARCODE_LATENT_IMAGE - Static variable in class com.datecs.barcode.Barcode
  LATENT IMAGE
BARCODE_MATRIX_2OF5 - Static variable in class com.datecs.barcode.Barcode
  MATRIX 2OF5
BARCODE_MAXICODE - Static variable in class com.datecs.barcode.Barcode
  MAXICODE
BARCODE_MICROPDF417 - Static variable in class com.datecs.barcode.Barcode
  MICROPDF417
BARCODE_MODE_MOTION_DETECT - Static variable in class com.datecs.linea.LineaPro
  Barcode engine into motion detect mode.
BARCODE_MODE_MULTI_SCAN - Static variable in class com.datecs.linea.LineaPro
  Barcode engine into multiple scan mode.
BARCODE_MODE_MULTI_SCAN_NO_DUPLICATE - Static variable in class com.datecs.linea.LineaPro
  Barcode engine into multiple scan mode with no duplicates.
BARCODE_MODE_SINGLE_SCAN - Static variable in class com.datecs.linea.LineaPro
  Barcode engine into single scan mode.
BARCODE_MODE_SINGLE_SCAN_ON_RELEASE - Static variable in class com.datecs.linea.LineaPro
  Barcode engine into single scan mode.
BARCODE_MSI_PLESSEY - Static variable in class com.datecs.barcode.Barcode
  MSI PLESSEY
BARCODE_PDF417 - Static variable in class com.datecs.barcode.Barcode
  PDF417
BARCODE_PDF417 - Static variable in class com.datecs.printer.Printer
  PDF417 barcode type.
BARCODE_PHARMACODE - Static variable in class com.datecs.barcode.Barcode
  PHARMACODE
BARCODE_PLANET - Static variable in class com.datecs.barcode.Barcode
  PLANET
BARCODE_POSTBAR - Static variable in class com.datecs.barcode.Barcode
  POSTBAR
BARCODE_POSTNET - Static variable in class com.datecs.barcode.Barcode
  POSTNET
BARCODE_QRCODE - Static variable in class com.datecs.barcode.Barcode
  QRCODE
BARCODE_RESERVED1 - Static variable in class com.datecs.barcode.Barcode
  RESERVED 1
BARCODE_RESERVED2 - Static variable in class com.datecs.barcode.Barcode
  RESERVED 2
BARCODE_RESERVED3 - Static variable in class com.datecs.barcode.Barcode
  RESERVED 3
BARCODE_RESERVED4 - Static variable in class com.datecs.barcode.Barcode
  RESERVED 4
BARCODE_RESERVED5 - Static variable in class com.datecs.barcode.Barcode
  RESERVED 5
BARCODE_RM4SCC - Static variable in class com.datecs.barcode.Barcode
  RM4SCC
BARCODE_SCODE - Static variable in class com.datecs.barcode.Barcode
  SCODE
BARCODE_TELEPEN - Static variable in class com.datecs.barcode.Barcode
  TELEPEN
BARCODE_UK_PLESSEY - Static variable in class com.datecs.barcode.Barcode
  UK PLESSEY
BARCODE_UNKNOWN - Static variable in class com.datecs.barcode.Barcode
  UNKNOWN
BARCODE_UPCA - Static variable in class com.datecs.barcode.Barcode
  UPCA
BARCODE_UPCA - Static variable in class com.datecs.printer.Printer
  UPC-A barcode type.
BARCODE_UPCA_2 - Static variable in class com.datecs.barcode.Barcode
  UPCA 2
BARCODE_UPCA_5 - Static variable in class com.datecs.barcode.Barcode
  UPCA 5
BARCODE_UPCE - Static variable in class com.datecs.barcode.Barcode
  UPCE
BARCODE_UPCE - Static variable in class com.datecs.printer.Printer
  UPC-E barcode type.
BARCODE_UPCE_2 - Static variable in class com.datecs.barcode.Barcode
  UPCE 2
BARCODE_UPCE_5 - Static variable in class com.datecs.barcode.Barcode
  UPCE 5
bcGetEngine() - Method in class com.datecs.linea.LineaPro
  Get barcode engine.
bcGetMode() - Method in class com.datecs.linea.LineaPro
  Get barcode scan mode.
bcGetTimeout() - Method in class com.datecs.linea.LineaPro
  Get barcode timeout.
bcRead() - Method in class com.datecs.linea.LineaPro
  Read data from barcode module.
bcRestoreDefaultMode() - Method in class com.datecs.linea.LineaPro
  Reset barcode scanner to default state.
bcSetBeep(int, int[]) - Method in class com.datecs.linea.LineaPro
  Set the sound to play sounds on barcode scan.
bcSetKeepAlive(boolean) - Method in class com.datecs.linea.LineaPro
  Set barcode scanner to be always ready for scanning and do not go to sleep state.
bcSetMode(int) - Method in class com.datecs.linea.LineaPro
  Set barcode scan mode.
bcSetTimeout(int) - Method in class com.datecs.linea.LineaPro
  Set barcode timeout.
bcStartScan() - Method in class com.datecs.linea.LineaPro
  Start barcode scanning.
bcStartUpdateMode(byte[]) - Method in class com.datecs.linea.LineaPro
  Set barcode scanner in firmware update mode.
bcStopBeep() - Method in class com.datecs.linea.LineaPro
  Stop play sounds on barcode scan.
bcStopScan() - Method in class com.datecs.linea.LineaPro
  Stop barcode scanning.
bcVendorInit(byte[]) - Method in class com.datecs.linea.LineaPro
  Set vendor specific initialization command to barcode scanner.
bcWrite(byte[]) - Method in class com.datecs.linea.LineaPro
  Write data to barcode module.
beep(int, int[]) - Method in class com.datecs.linea.LineaPro
  Play sounds on device speaker.
beep(int, int, int) - Method in class com.datecs.linea.LineaPro
  Play sounds on device speaker.
beep() - Method in class com.datecs.printer.Printer
  Sounds the buzzer.
blockSize - Variable in class com.datecs.rfid.ContactlessCard
  The card block size (Available for ISO15 cards only).
BUILD_DATE - Static variable in class com.datecs.BuildInfo
  The user-visible date string in format 'yyyyMMddHHmmss'.
BUILD_NUMBER - Static variable in class com.datecs.BuildInfo
  The build number of the product.
BuildInfo - Class in com.datecs
  Information about the current build.
BuildInfo() - Constructor for class com.datecs.BuildInfo
BUTTON_MODE_BARCODE - Static variable in class com.datecs.universalreader.UniversalReader
BUTTON_MODE_NONE - Static variable in class com.datecs.universalreader.UniversalReader
BUTTON_MODE_STATUS - Static variable in class com.datecs.universalreader.UniversalReader

## C

calculate(byte[], int, int) - Static method in class com.datecs.crypto.SHA1
calculate(byte[]) - Static method in class com.datecs.crypto.SHA1
calculate(ByteBuffer) - Static method in class com.datecs.crypto.SHA1
calculate(byte[], int, int) - Static method in class com.datecs.crypto.SHA256
calculate(byte[]) - Static method in class com.datecs.crypto.SHA256
calculate(ByteBuffer) - Static method in class com.datecs.crypto.SHA256
calibrateBMMSensor() - Method in class com.datecs.printer.Printer
  Black mark mode sensor calibration.
CAPABILITY_BARCODE - Static variable in class com.datecs.universalreader.UniversalReader
  Barcode reader capability.
CAPABILITY_BUTTON - Static variable in class com.datecs.universalreader.UniversalReader
  Button capability.
CAPABILITY_DEBUG - Static variable in class com.datecs.universalreader.UniversalReader
  Debug version capability.
CAPABILITY_EV15 - Static variable in class com.datecs.universalreader.UniversalReader
  Barcode reader EV15 capability.
CAPABILITY_FIRMWARE - Static variable in class com.datecs.universalreader.UniversalReader
  Firmware download capability.
CAPABILITY_GSM - Static variable in class com.datecs.universalreader.UniversalReader
  GSM module capability.
CAPABILITY_LCD2X16 - Static variable in class com.datecs.universalreader.UniversalReader
  LCD 2x16 capability.
CAPABILITY_MAGNETIC - Static variable in class com.datecs.universalreader.UniversalReader
  Magnetic reader capability.
CAPABILITY_MIFARE - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare reader capability.
CAPABILITY_SMARTCARD - Static variable in class com.datecs.universalreader.UniversalReader
  Smart card reader capability.
CAPABILITY_TOUCHSCREEN - Static variable in class com.datecs.universalreader.UniversalReader
  Touch screen capability.
capacity - Variable in class com.datecs.rfid.ContactlessCard
  The card capacity.
CARD_EPASSPORT - Static variable in class com.datecs.rfid.ContactlessCard
  E Passport.
CARD_FELICA - Static variable in class com.datecs.rfid.ContactlessCard
  FeliCa
CARD_ISO14443A - Static variable in class com.datecs.rfid.ContactlessCard
  ISO 14443A.
CARD_ISO14443B - Static variable in class com.datecs.rfid.ContactlessCard
  ISO 14443B.
CARD_ISO15693 - Static variable in class com.datecs.rfid.ContactlessCard
  ISO 15693.
CARD_MIFARE_CLASSIC_1K - Static variable in class com.datecs.rfid.ContactlessCard
  Mifare Classic 1K.
CARD_MIFARE_CLASSIC_4K - Static variable in class com.datecs.rfid.ContactlessCard
  Mifare Classic 4K.
CARD_MIFARE_DESFIRE - Static variable in class com.datecs.rfid.ContactlessCard
  Mifare Desfire.
CARD_MIFARE_MINI - Static variable in class com.datecs.rfid.ContactlessCard
  Mifare Mini.
CARD_MIFARE_PLUS - Static variable in class com.datecs.rfid.ContactlessCard
  Mifare Plus.
CARD_MIFARE_ULTRALIGHT - Static variable in class com.datecs.rfid.ContactlessCard
  Mifare Ultralight.
CARD_MIFARE_ULTRALIGHT_C - Static variable in class com.datecs.rfid.ContactlessCard
  Mifare Ultralight C.
CARD_PAYMENT - Static variable in class com.datecs.rfid.ContactlessCard
  Payment card.
CARD_PICOPASS_14443B - Static variable in class com.datecs.rfid.ContactlessCard
  PicoPass 15693.
CARD_PICOPASS_15693 - Static variable in class com.datecs.rfid.ContactlessCard
  PicoPass 15693.
CARD_ST_SRI - Static variable in class com.datecs.rfid.ContactlessCard
  ST SRI
CARD_SUPPORT_FELICA - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_FELICA - Static variable in class com.datecs.rfid.RFID
  FeliCa card.
CARD_SUPPORT_ISO15 - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_ISO15 - Static variable in class com.datecs.rfid.RFID
  ISO15 card.
CARD_SUPPORT_JEWEL - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_JEWEL - Static variable in class com.datecs.rfid.RFID
  JEWEL card.
CARD_SUPPORT_NFC - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_NFC - Static variable in class com.datecs.rfid.RFID
  NFC card.
CARD_SUPPORT_PICOPASS_ISO14 - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_PICOPASS_ISO15 - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_STSRI - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_STSRI - Static variable in class com.datecs.rfid.RFID
  ST SRI card.
CARD_SUPPORT_TYPE_A - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_TYPE_A - Static variable in class com.datecs.rfid.RFID
  TYPE A card.
CARD_SUPPORT_TYPE_B - Static variable in class com.datecs.rfid.RC663
CARD_SUPPORT_TYPE_B - Static variable in class com.datecs.rfid.RFID
  TYPE B card.
CARD_UNKNOWN - Static variable in class com.datecs.rfid.ContactlessCard
  Unknown card.
ccit16(int, byte[], int, int) - Static method in class com.datecs.crypto.CRC
ccit16(int, byte[]) - Static method in class com.datecs.crypto.CRC
ccit16(byte[], int, int) - Static method in class com.datecs.crypto.CRC
channel - Variable in class com.datecs.rfid.ContactlessCard
  The card channel.
CHANNEL_EMSR - Static variable in class com.datecs.printer.ProtocolAdapter
CHANNEL_FELICA - Static variable in class com.datecs.rfid.RC663
  FELICA channel.
CHANNEL_ISO1443A - Static variable in class com.datecs.rfid.RC663
  ISO1443A channel.
CHANNEL_ISO1443B - Static variable in class com.datecs.rfid.RC663
  ISO1443B channel.
CHANNEL_ISO15693 - Static variable in class com.datecs.rfid.RC663
  ISO15693 channel.
CHANNEL_MAIN - Static variable in class com.datecs.rfid.RC663
  Main channel.
CHANNEL_PRINTER - Static variable in class com.datecs.printer.ProtocolAdapter
  The channel associated with printer hardware module.
CHANNEL_RFID - Static variable in class com.datecs.printer.ProtocolAdapter
  The channel associated with RFID reader.
CHANNEL_STSRI - Static variable in class com.datecs.rfid.RC663
  ST SRI channel.
CHANNEL_UNIVERSAL_READER - Static variable in class com.datecs.printer.ProtocolAdapter
  The channel associated with Universal Reader hardware module.
checkIdentity() - Method in class com.datecs.biometric.TouchChip
  Check an identify.
close() - Method in class com.datecs.drawer.Drawer
  Close the streams and release all associated resources.
close() - Method in class com.datecs.emsr.EMSR
  Close the streams and release all associated resources.
close() - Method in class com.datecs.hub.Hub
close() - Method in class com.datecs.linea.LineaPro
  Close the streams and release all associated resources.
close() - Method in class com.datecs.printer.Printer
  Close the streams and release all associated resources.
close() - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Close channel.
close() - Method in class com.datecs.printer.ProtocolAdapter
  Close the streams and release all associated resources.
close() - Method in class com.datecs.rfid.RFID
  Close attached streams and release associated resources.
close() - Method in class com.datecs.universalreader.UniversalReader
  Close the streams and release all associated resources.
com.datecs - package com.datecs
com.datecs.barcode - package com.datecs.barcode
com.datecs.biometric - package com.datecs.biometric
com.datecs.card - package com.datecs.card
com.datecs.crypto - package com.datecs.crypto
com.datecs.drawer - package com.datecs.drawer
com.datecs.emsr - package com.datecs.emsr
com.datecs.hub - package com.datecs.hub
com.datecs.linea - package com.datecs.linea
com.datecs.printer - package com.datecs.printer
com.datecs.rfid - package com.datecs.rfid
com.datecs.smartcard - package com.datecs.smartcard
com.datecs.universalreader - package com.datecs.universalreader
completion() - Method in class com.datecs.rfid.STSRICard
  Card completion.
config() - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Configures Mifare card reader.
ContactlessCard - Class in com.datecs.rfid
  This class represents basic functionality of contactless card.
ContactlessCard(RC663) - Constructor for class com.datecs.rfid.ContactlessCard
  Create a new instance of this class.
CRC - Class in com.datecs.crypto
  Helper methods for CRC calculations.
CRC() - Constructor for class com.datecs.crypto.CRC
create(byte[], String, String, String, String, String, byte[], byte[]) - Static method in class com.datecs.crypto.TR31
create(byte[], String, String, String, String, String, byte[]) - Static method in class com.datecs.crypto.TR31
create(byte[]) - Static method in class com.datecs.linea.LineaPro.BatteryInfo
  Create instance of this class from binary data.
create(byte[]) - Static method in class com.datecs.linea.LineaProInformation
  Create instance of this class from binary data.
createAES(long, byte[], String, String, String, String, String, byte[], byte[]) - Static method in class com.datecs.crypto.TR31
createAES(byte[], String, String, String, String, String, byte[], byte[]) - Static method in class com.datecs.crypto.TR31
createAES(byte[], String, String, String, String, String, byte[]) - Static method in class com.datecs.crypto.TR31
createDerivationData(DUKPT.DerivationPurpose, DUKPT.KeyUsage, DUKPT.KeyType, byte[], int) - Static method in class com.datecs.crypto.DUKPT
createFile(int, int, int, int, int) - Method in class com.datecs.rfid.ISO14443Card.DESFire
cutPaper(int, int) - Method in class com.datecs.printer.Printer
  Cut paper.
cutPaper() - Method in class com.datecs.printer.Printer
  Cut paper.

## D

decrement(int, int, int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Performs value decrement operation in Mifare card.
decrypt(byte[], byte[], byte[]) - Static method in class com.datecs.crypto.RSA
  Decrypt data
decryptCBC(byte[], byte[], byte[]) - Static method in class com.datecs.crypto.AES
  Decrypt data using CBC mode.
decryptCBC(byte[], byte[]) - Static method in class com.datecs.crypto.AES
  Decrypt data using CBC mode and zero initialization vector.
decryptCBC(byte[], byte[], byte[]) - Static method in class com.datecs.crypto.TripleDES
  Decrypt data using CBC mode.
decryptCBC(byte[], byte[], byte[], int, int) - Static method in class com.datecs.crypto.TripleDES
  Decrypt data using CBC mode.
decryptCBC(byte[], byte[]) - Static method in class com.datecs.crypto.TripleDES
  Decrypt data using CBC mode.
decryptCBC(byte[], byte[], int, int) - Static method in class com.datecs.crypto.TripleDES
  Decrypt data using CBC mode.
decryptECB(byte[], byte[]) - Static method in class com.datecs.crypto.AES
  Decrypt data using ECB mode.
decryptECB(byte[], byte[]) - Static method in class com.datecs.crypto.TripleDES
  Decrypt data using ECB mode.
deinitialise() - Method in class com.datecs.rfid.ContactlessCard
  Deinitialise card.
deinitialise() - Method in class com.datecs.rfid.FeliCaCard
deinitialise() - Method in class com.datecs.rfid.ISO14443Card
deinitialise() - Method in class com.datecs.rfid.ISO15693Card
deinitialise() - Method in class com.datecs.rfid.STSRICard
deleteIdentity(int) - Method in class com.datecs.biometric.TouchChip
  Delete an already enrolled template at a specified slot in the TouchChip module non-volatile memory.
deriveDataKey(byte[], byte[]) - Static method in class com.datecs.crypto.DUKPT
deriveInitialKey(byte[], DUKPT.KeyType, byte[]) - Static method in class com.datecs.crypto.DUKPT
deriveIpek(byte[], byte[]) - Static method in class com.datecs.crypto.DUKPT
deriveKey(byte[], byte[]) - Static method in class com.datecs.crypto.DUKPT
deriveKey(byte[], DUKPT.KeyType, byte[]) - Static method in class com.datecs.crypto.DUKPT
deriveKey(byte[], byte[]) - Static method in class com.datecs.crypto.TR31
deriveMacKey(byte[], byte[]) - Static method in class com.datecs.crypto.DUKPT
derivePinKey(byte[], byte[]) - Static method in class com.datecs.crypto.DUKPT
deriveWorkingKey(byte[], DUKPT.KeyType, DUKPT.KeyUsage, DUKPT.KeyType, byte[], int) - Static method in class com.datecs.crypto.DUKPT
deriveWorkingKey(byte[], DUKPT.KeyType, DUKPT.KeyUsage, DUKPT.KeyType, byte[]) - Static method in class com.datecs.crypto.DUKPT
DESFire() - Method in class com.datecs.rfid.ISO14443Card
DESFire() - Constructor for class com.datecs.rfid.ISO14443Card.DESFire
disable() - Method in class com.datecs.emsr.EMSR
  Disable encrypted magnetic stripe reader (EMSR).
disable() - Method in class com.datecs.rfid.RC663
  Powers on the RF card reader module and release associated resources.
displayText(String, String) - Method in class com.datecs.universalreader.UniversalReader
  Display text.
Drawer - Class in com.datecs.drawer
  Created by lkm on 8.9.2017 г..
Drawer(InputStream, OutputStream) - Constructor for class com.datecs.drawer.Drawer
  Constructs a new instance of this class from a given streams.
Drawer.ConnectionListener - Interface in com.datecs.drawer
  This interface is used to notify when connection state is changed.
Drawer.StateListener - Interface in com.datecs.drawer
  This interface is used to notify when device state is changed.
drawPageFrame(int, int, int, int, int, int) - Method in class com.datecs.printer.Printer
  Draws a rectangle frame with selected thickness in page mode.
drawPageRectangle(int, int, int, int, int) - Method in class com.datecs.printer.Printer
  Draws a rectangle in page mode.
dsfid - Variable in class com.datecs.rfid.ContactlessCard
  The card data storage format identifier (Available for ISO15 cards only).
DUKPT - Class in com.datecs.crypto
  Helper methods for DUKPT key generation.
DUKPT() - Constructor for class com.datecs.crypto.DUKPT
DUKPT.DerivationPurpose - Enum in com.datecs.crypto
  Identifies if this derivation is to create an initial key or any other key type to help select which derivation data table to use.
DUKPT.KeyType - Enum in com.datecs.crypto
  KeyType defines the cryptographic key type being derived.
DUKPT.KeyUsage - Enum in com.datecs.crypto
  KeyUsage defines the possible key usages that can be derived.

## E

EMSR - Class in com.datecs.emsr
EMSR(InputStream, OutputStream) - Constructor for class com.datecs.emsr.EMSR
  Constructs a new instance of this class from a given `InputStream` and `OutputStream`.
EMSR.EMSRInformation - Class in com.datecs.emsr
  The class that contains various information about encrypted magnetic stripe reader (EMSR).
EMSR.EMSRKeyInformation - Class in com.datecs.emsr
  The class that contains various information about encrypted magnetic stripe reader (EMSR).
EMSRException - Exception in com.datecs.emsr
  Encrypted magnetic stripe reader exception class.
EMSRException(int) - Constructor for exception com.datecs.emsr.EMSRException
  Create a new instance of `EMSRException` class.
enable() - Method in class com.datecs.emsr.EMSR
  Enable encrypted magnetic stripe reader (EMSR).
enable() - Method in class com.datecs.rfid.RC663
  Initializes and powers on the RF card reader module.
enableAustralianPost(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Australian Post.
enableAztec(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Aztec.
enableBatteryCharge(boolean) - Method in class com.datecs.linea.LineaPro
  Enable mobile device battery charge when device is not powered.
enableCodabarl(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Codabar.
enableCodablockA(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable CodablockA.
enableCodablockF(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable CodablockF.
enableCode11(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Code 11.
enableCode128(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Code 128.
enableCode39(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Code 39.
enableCode93(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Code 93.
enableDataMatrix(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable DataMatrix.
enableDutchPost(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Dutch Post.
enableEAN13(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable EAN-13.
enableEAN8(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable EAN-8.
enableEvents(boolean) - Method in class com.datecs.drawer.Drawer
  Open drawer with default impulse (30).
enableExternalSpeaker(boolean) - Method in class com.datecs.linea.LineaPro
  Enable external speaker as default audio source.
enableExternalSpeakerButton(boolean) - Method in class com.datecs.linea.LineaPro
  Enable external speaker button.
enableGlareDetection(boolean) - Method in class com.datecs.barcode.Intermec
  Turn glare detection on and off.
enableGS1(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable GS1-128.
enableGS1CompositeAorB(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable GS1 Composite A/B.
enableGS1CompositeC(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable GS1 Composite C..
enableGS1DatabarExpanded(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable GS1 DataBar Expanded.
enableGS1DatabarLimited(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable GS1 DataBar Limited.
enableInfomail(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable British Royal Mail Infomail symbology.
enableInterleaved2of5(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Interleaved 2 of 5.
enableISBT(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable ISBT.
enableJapanPost(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Japan Post.
enableMagneticCardReader(boolean) - Method in class com.datecs.universalreader.UniversalReader
  Enables magnetic card reader.
enableMagneticCardReaderEvents(boolean) - Method in class com.datecs.universalreader.UniversalReader
enableMatrix2of5(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Matrix 2 of 5.
enableMaxCurrent(boolean) - Method in class com.datecs.linea.LineaPro
  Enable max current throughput for the gang charger.
enableMaxicode(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Maxicode.
enableMicroPDF417(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Micro PDF417.
enableMSICode(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable MSI Code.
enableMulticode(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Multicode.
enablePDF417(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable PDF417.
enablePlanet(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Planet.
enablePlesseyCode(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Plessey Code.
enablePostnet(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Postnet.
enableQRCode(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable QR Code.
enableRSS14(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable RSS 14.
enableScanButton(boolean) - Method in class com.datecs.linea.LineaPro
  Enable or disable device scan button.
enableStandard2of5(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Standard 2 of 5.
enableSymbology(int, int, boolean) - Method in class com.datecs.barcode.Intermec
  Enable barcode symbology.
enableTelepen(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable Telepen.
enableTLC39(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable TLC 39.
enableUPCA(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable UPC-A.
enableUPCE(boolean) - Method in class com.datecs.barcode.Intermec
  Enable or disable UPC-E.
encrypt(byte[], byte[], byte[]) - Static method in class com.datecs.crypto.RSA
  Encrypt data
encryptCBC(byte[], byte[], byte[]) - Static method in class com.datecs.crypto.AES
  Encrypt data using CBC mode.
encryptCBC(byte[], byte[]) - Static method in class com.datecs.crypto.AES
  Encrypt data using CBC mode and zero initialization vector.
encryptCBC(byte[], byte[], byte[]) - Static method in class com.datecs.crypto.TripleDES
  Encrypt data using CBC mode.
encryptCBC(byte[], byte[]) - Static method in class com.datecs.crypto.TripleDES
  Encrypt data using CBC mode.
encryptECB(byte[], byte[]) - Static method in class com.datecs.crypto.AES
  Encrypt data using ECB mode.
encryptECB(byte[], byte[]) - Static method in class com.datecs.crypto.TripleDES
  Encrypt data using ECB mode.
ENCRYPTION_TYPE_AES256 - Static variable in class com.datecs.emsr.EMSR
  Encrypted Magnetic Head AES 256 encryption algorithm After decryption, the result data will be as follows: Random data (4 bytes).
ENCRYPTION_TYPE_IDTECH - Static variable in class com.datecs.emsr.EMSR
  Encrypted Magnetic Head IDTECH encryption algorithm, please refer to IDTECH documentation for detailed format and examples.
ENCRYPTION_TYPE_OLD_RSA - Static variable in class com.datecs.emsr.EMSR
  Card data will be sent encrypted in the format: Encryption type (1 byte): 01 - RSA2048 encrypted.
ENCRYPTION_TYPE_RSA - Static variable in class com.datecs.emsr.EMSR
  Card data will be sent encrypted in the format: Encryption type (1 byte): 01 - RSA2048 encrypted.
enrolIdentity(byte[]) - Method in class com.datecs.biometric.TouchChip
  Enrol finger print template in the TouchChip module non-volatile memory.
enrolIdentity(String) - Method in class com.datecs.biometric.TouchChip
  Enrol finger print template in the TouchChip module non-volatile memory.
ERROR_0K - Static variable in class com.datecs.universalreader.UniversalReader
  Operation successful.
ERROR_BARCODE - Static variable in class com.datecs.universalreader.UniversalReader
  Barcode reader communication error.
ERROR_BARCODE_INVALID - Static variable in class com.datecs.universalreader.UniversalReader
  Barcode reader invalid command.
ERROR_BARCODE_NODATA - Static variable in class com.datecs.universalreader.UniversalReader
  No barcode read.
ERROR_BARCODE_NOTPRESENT - Static variable in class com.datecs.universalreader.UniversalReader
  Barcode reader not present.
ERROR_BUSY - Static variable in exception com.datecs.linea.LineaProException
  Busy.
ERROR_CARD - Static variable in class com.datecs.universalreader.UniversalReader
  Card error.
ERROR_COM - Static variable in exception com.datecs.linea.LineaProException
  COM error.
ERROR_COMMUNICATION - Static variable in class com.datecs.hub.Hub
  Communication error.
ERROR_CONFIG - Static variable in exception com.datecs.linea.LineaProException
  Configuration error.
ERROR_CRYPT - Static variable in exception com.datecs.linea.LineaProException
  Crypt error.
ERROR_EMV - Static variable in exception com.datecs.linea.LineaProException
  EMV error.
ERROR_FAILED - Static variable in exception com.datecs.rfid.RFIDException
  Command failed.
ERROR_FIRST_DATA - Static variable in exception com.datecs.linea.LineaProException
  First data.
ERROR_FLASH - Static variable in exception com.datecs.linea.LineaProException
  Flash error.
ERROR_GENERAL - Static variable in exception com.datecs.linea.LineaProException
  General error.
ERROR_INVALID - Static variable in class com.datecs.universalreader.UniversalReader
  Invalid command code.
ERROR_INVALID_AUTH - Static variable in exception com.datecs.linea.LineaProException
  Invalid authentication.
ERROR_INVALID_COMMAND - Static variable in class com.datecs.hub.Hub
  Invalid command INS.
ERROR_INVALID_COMMAND - Static variable in exception com.datecs.linea.LineaProException
  Invalid command.
ERROR_INVALID_KEY - Static variable in exception com.datecs.linea.LineaProException
  Invalid key.
ERROR_INVALID_LENGTH - Static variable in class com.datecs.hub.Hub
  Wrong data field length.
ERROR_INVALID_LENGTH - Static variable in exception com.datecs.linea.LineaProException
  Invalid length.
ERROR_INVALID_VALUE - Static variable in exception com.datecs.linea.LineaProException
  Invalid value.
ERROR_LAST_DATA - Static variable in exception com.datecs.linea.LineaProException
  Last data.
ERROR_MIFARE_ACCESS - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare access error.
ERROR_MIFARE_AUTHENTICATION - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare authentication error.
ERROR_MIFARE_BIT - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare bit count error.
ERROR_MIFARE_CODE - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare code error.
ERROR_MIFARE_COLLISION - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare collision error.
ERROR_MIFARE_CRC - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare CRC error.
ERROR_MIFARE_EACCESS - Static variable in exception com.datecs.rfid.RFIDException
  Mifare access error.
ERROR_MIFARE_EAUTHENTICATION - Static variable in exception com.datecs.rfid.RFIDException
  Mifare authentication error.
ERROR_MIFARE_EBASE - Static variable in exception com.datecs.rfid.RFIDException
  Mifare operation successful.
ERROR_MIFARE_EBIT - Static variable in exception com.datecs.rfid.RFIDException
  Mifare bit count error.
ERROR_MIFARE_ECODE - Static variable in exception com.datecs.rfid.RFIDException
  Mifare code error.
ERROR_MIFARE_ECOLLISION - Static variable in exception com.datecs.rfid.RFIDException
  Mifare collision error.
ERROR_MIFARE_ECRC - Static variable in exception com.datecs.rfid.RFIDException
  Mifare CRC error.
ERROR_MIFARE_EEEPROM - Static variable in exception com.datecs.rfid.RFIDException
  Mifare EEPROM error.
ERROR_MIFARE_EEPROM - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare EEPROM error.
ERROR_MIFARE_EFIFO - Static variable in exception com.datecs.rfid.RFIDException
  Mifare FIFO overflow.
ERROR_MIFARE_EFRAME - Static variable in exception com.datecs.rfid.RFIDException
  Mifare frame error.
ERROR_MIFARE_EGENERIC - Static variable in exception com.datecs.rfid.RFIDException
  Mifare generic error.
ERROR_MIFARE_EKEY - Static variable in exception com.datecs.rfid.RFIDException
  Mifare invalid key.
ERROR_MIFARE_EPARITY - Static variable in exception com.datecs.rfid.RFIDException
  Mifare parity error.
ERROR_MIFARE_ETIMEOUT - Static variable in exception com.datecs.rfid.RFIDException
  Mifare timeout error.
ERROR_MIFARE_EVALUE - Static variable in exception com.datecs.rfid.RFIDException
  Mifare value error.
ERROR_MIFARE_FIFO - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare FIFO overflow.
ERROR_MIFARE_FRAME - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare frame error.
ERROR_MIFARE_GENERIC - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare generic error.
ERROR_MIFARE_KEY - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare invalid key.
ERROR_MIFARE_PARITY - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare parity error.
ERROR_MIFARE_TIMEOUT - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare timeout error.
ERROR_MIFARE_VALUE - Static variable in class com.datecs.universalreader.UniversalReader
  Mifare value error.
ERROR_NO - Static variable in exception com.datecs.linea.LineaProException
  No error.
ERROR_NO_DATA - Static variable in exception com.datecs.linea.LineaProException
  No data.
ERROR_NO_PERM - Static variable in exception com.datecs.linea.LineaProException
  No permission.
ERROR_NODATA - Static variable in class com.datecs.universalreader.UniversalReader
  No data available.
ERROR_NORESPONCE - Static variable in class com.datecs.universalreader.UniversalReader
  No response from device.
ERROR_NOTPERMITTED - Static variable in class com.datecs.universalreader.UniversalReader
  Command not permitted.
ERROR_NVRAM - Static variable in class com.datecs.hub.Hub
  Error with NV memory.
ERROR_OUT_OF_MEMORY - Static variable in exception com.datecs.linea.LineaProException
  Out of memory.
ERROR_SLAVE - Static variable in class com.datecs.hub.Hub
  Slave ID is not available.
ERROR_SYNTAX - Static variable in class com.datecs.universalreader.UniversalReader
  Syntax error.
ERROR_TAMPERED - Static variable in exception com.datecs.linea.LineaProException
  Tampered.
ERROR_TIMEOUT - Static variable in class com.datecs.hub.Hub
  Timeout occurred during command reception.
ERROR_TIMEOUT - Static variable in exception com.datecs.linea.LineaProException
  Timeout.
ERROR_TIMEOUT - Static variable in exception com.datecs.rfid.RFIDException
  Timeout expired.
EVENT_SLAVE_CONNECTED - Static variable in class com.datecs.hub.Hub
EVENT_SLAVE_DATA_RECEIVED - Static variable in class com.datecs.hub.Hub
EVENT_SLAVE_DISCONNECTED - Static variable in class com.datecs.hub.Hub
EVENT_SLAVE_OVERCURRENT - Static variable in class com.datecs.hub.Hub
executeAPDU(int, int, int, int, byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Execute APDU command.
executeAPDU(int, int, int, int, byte[], int) - Method in class com.datecs.rfid.ISO14443Card
  Execute APDU command.

## F

feedLabel() - Method in class com.datecs.printer.Printer
  Feed to the next label.
feedPaper(int) - Method in class com.datecs.printer.Printer
  Feeds paper with specified lines number.
FELICA_SMARTTAG_BATTERY_LOW1 - Static variable in class com.datecs.rfid.FeliCaCard
  Low, consider replacing.
FELICA_SMARTTAG_BATTERY_LOW2 - Static variable in class com.datecs.rfid.FeliCaCard
  Very Low, replace it.
FELICA_SMARTTAG_BATTERY_NORMAL1 - Static variable in class com.datecs.rfid.FeliCaCard
  Normal, card can be used.
FELICA_SMARTTAG_BATTERY_NORMAL2 - Static variable in class com.datecs.rfid.FeliCaCard
  Normal, card can be used.
FELICA_SMARTTAG_DRAW_BLACK_BACKGROUND - Static variable in class com.datecs.rfid.FeliCaCard
  The area outside of the image will be shown black.
FELICA_SMARTTAG_DRAW_KEEP_BACKGROUND - Static variable in class com.datecs.rfid.FeliCaCard
  The area outside of the image will be kept to its current state.
FELICA_SMARTTAG_DRAW_USE_LAYOUT - Static variable in class com.datecs.rfid.FeliCaCard
  The area outside of the image will be drawn using one of the previously stored layouts.
FELICA_SMARTTAG_DRAW_WHITE_BACKGROUND - Static variable in class com.datecs.rfid.FeliCaCard
  The area outside of the image will be emptied.
FeliCaCard - Class in com.datecs.rfid
FeliCaCard(RC663) - Constructor for class com.datecs.rfid.FeliCaCard
  Constructs a new instance of this class.
FILL_BLACK - Static variable in class com.datecs.printer.Printer
  The area is filled (black color).
FILL_INVERTED - Static variable in class com.datecs.printer.Printer
  The area is inverted.
FILL_WHITE - Static variable in class com.datecs.printer.Printer
  The area is cleared (white color).
FinancialCard - Class in com.datecs.card
  This class represents an extracted account information from financial card track data.
FinancialCard(String) - Constructor for class com.datecs.card.FinancialCard
  Constructs a new instance of this class from a given financial card track data.
flush() - Method in class com.datecs.printer.Printer
  Flushes the output stream and forces any buffered output bytes to be written out.
flush(boolean) - Method in class com.datecs.printer.Printer
  Flushes the output stream and forces any buffered output bytes to be written out.
fwErase() - Method in class com.datecs.linea.LineaPro
  Erase current firmware.
fwStart() - Method in class com.datecs.linea.LineaPro
  Start firmware update.
fwStop() - Method in class com.datecs.linea.LineaPro
  End firmware update.
fwUpdate(byte[]) - Method in class com.datecs.linea.LineaPro
  Update firmware.
fwWrite(int, byte[]) - Method in class com.datecs.linea.LineaPro
  Write firmware chunk.

## G

getAction() - Method in class com.datecs.universalreader.TouchEvent
  Gets the kind of action being performed.
getATS() - Method in class com.datecs.rfid.ISO14443Card
  Get ATS.
getAttribB(int, int, int, int) - Method in class com.datecs.rfid.ISO14443Card
  Get attribute B
getAutoOffTime(boolean) - Method in class com.datecs.linea.LineaPro
  Get the time after which the device shall automatically goes off.
getAverageCurrent() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get average current in mA.
getAveragePower() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get average power in mW.
getBarcodeReader() - Method in class com.datecs.universalreader.UniversalReader
  Returns an instance of `BarcodeReader` class.
getBatteryInfo() - Method in class com.datecs.linea.LineaPro
  Get extended battery information.
getBatteryLevel() - Method in class com.datecs.linea.LineaPro
  Return device battery level.
getBatteryVoltage() - Method in class com.datecs.linea.LineaPro
  Return device battery voltage.
getBlocksSecurityStatus(int, int) - Method in class com.datecs.rfid.ISO15693Card
  Reads the security status of one more more blocks from ISO 15693 card.
getBytes() - Method in class com.datecs.smartcard.AnswerToReset
  Returns a copy of the bytes in this ATR.
getBytes() - Method in class com.datecs.smartcard.ResponseAPDU
  Returns a copy of the bytes in this APDU.
getCapabilities() - Method in class com.datecs.universalreader.UniversalReader
  Gets device capabilities.
getCapacity() - Method in class com.datecs.linea.LineaPro.BatteryInfo
  Get battery capacity in %.
getCaptureDeviceID() - Method in class com.datecs.biometric.AnsiIso
  Get capture device ID.
getCaptureDeviceIDAsHexString() - Method in class com.datecs.biometric.AnsiIso
  Get capture device ID as HEX String.
getChannel() - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Gets the channel number.
getChannel(int) - Method in class com.datecs.printer.ProtocolAdapter
  Gets an instance of `ProtocolAdapter.Channel` from specified channel number.
getCountOfViews() - Method in class com.datecs.biometric.AnsiIso
  Get count of views.
getData() - Method in class com.datecs.barcode.Barcode
  Get barcode data.
getData() - Method in class com.datecs.biometric.AnsiIso
  Get finger image record data.
getData() - Method in class com.datecs.biometric.TouchChip.Template
getData() - Method in class com.datecs.linea.LineaPro.BatteryInfo
  Get the creation data.
getData() - Method in class com.datecs.linea.LineaProInformation
  Get the creation data.
getData() - Method in class com.datecs.printer.PrinterInformation
  Returns a copy of the information data as returned from printer.
getData() - Method in class com.datecs.smartcard.AnswerToReset
  Returns a copy of the data bytes in the response body.
getData() - Method in class com.datecs.smartcard.ResponseAPDU
  Returns a copy of the data bytes in the response body.
getDataInputStream(int) - Method in class com.datecs.hub.Hub
  Returns instance of InputStream associated with slave.
getDataOutputStream(int) - Method in class com.datecs.hub.Hub
  Returns instance of OutputStream associated with slave.
getDataString() - Method in class com.datecs.barcode.Barcode
  Get barcode data as string.
getDeviceMode() - Method in class com.datecs.linea.LineaPro
  Get the device mode.
getElapse() - Method in class com.datecs.universalreader.TouchEvent
  Gets the time between this event and the previous one.
getErrorCode() - Method in exception com.datecs.biometric.TouchChipException
  Retrieves the exception error code for this instance.
getErrorCode() - Method in exception com.datecs.hub.HubException
getErrorCode() - Method in exception com.datecs.linea.LineaProException
  Gets the error code that raise the exception.
getErrorCode() - Method in exception com.datecs.rfid.RFIDException
  Gets the error code that raise the exception.
getErrorCode() - Method in exception com.datecs.universalreader.UniversalReaderException
  Retrieves the exception error code for this instance.
getEvents() - Method in class com.datecs.universalreader.UniversalReader.TouchScreen
  Returns an instance of `TouchEvent[]`.
getExpiryMonth() - Method in class com.datecs.card.FinancialCard
  Returns an expiration month of this financial card.
getExpiryYear() - Method in class com.datecs.card.FinancialCard
  Returns an expiration year of this financial card.
getFeedLines() - Method in class com.datecs.printer.PrinterInformation
  Returns the number of dot lines needed to feed last printed line to cutter in.
getFingerDataBlockLength() - Method in class com.datecs.biometric.AnsiIso
  Get finger data block length.
getFingerImageQuality() - Method in class com.datecs.biometric.AnsiIso
  Get finger/palm image quality.
getFingerPosition() - Method in class com.datecs.biometric.AnsiIso
  Get finger position.
getFirmwareVersion() - Method in class com.datecs.printer.PrinterInformation
  Returns the printer firmware version.
getFirmwareVersionString() - Method in class com.datecs.printer.PrinterInformation
  Returns the printer firmware version as string.
getFormat() - Method in class com.datecs.biometric.TouchChip.Template
getFormatIdentifier() - Method in class com.datecs.biometric.AnsiIso
  Get format identifier.
getFormatIdentifierAsString() - Method in class com.datecs.biometric.AnsiIso
  Get format identifier as String.
getFuelgauge() - Method in class com.datecs.linea.LineaPro.BatteryInfo
  Get fuel gauge information.
getFullAvailableCapacity() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get full available capacity in mAh.
getFullChargeCapacity() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get full charge capacity in mAh.
getHeader() - Method in class com.datecs.biometric.AnsiIso
  Get finger image record header data.
getHeaderAsHexString() - Method in class com.datecs.biometric.AnsiIso
  Get finger image record header data as HEX string.
getHealthLevel() - Method in class com.datecs.linea.LineaPro.BatteryInfo
  Get battery health level in %.
getHorizontalLineLength() - Method in class com.datecs.biometric.AnsiIso
  Get horizontal line length (image width).
getIdent() - Method in class com.datecs.barcode.Intermec
getIdentification() - Method in class com.datecs.universalreader.UniversalReader
  Gets the device identification string.
getIdentity(int, int, int, TouchChip.ImageReceiver) - Method in class com.datecs.biometric.TouchChip
  Gets a finger print data in different formats.
getIdentity() - Method in class com.datecs.biometric.TouchChip.Identity
  Get identity data.
getIdentityAsString() - Method in class com.datecs.biometric.TouchChip.Identity
  Get identity data.
getImageAsquisionLevel() - Method in class com.datecs.biometric.AnsiIso
  Get acquisition level.
getImageCompressionAlgorithm() - Method in class com.datecs.biometric.AnsiIso
  Get compression algorithm.
getImageData() - Method in class com.datecs.biometric.AnsiIso
  Get finger/palm image data.
getImageResolutionHorz() - Method in class com.datecs.biometric.AnsiIso
  Get image resolution (horizontal).
getImageResolutionVert() - Method in class com.datecs.biometric.AnsiIso
  Get image resolution (vertical).
getImpressionType() - Method in class com.datecs.biometric.AnsiIso
  Get impression type.
getInformation() - Method in class com.datecs.emsr.EMSR
  Returns information about encrypted magnetic stripe reader (EMSR).
getInformation() - Method in class com.datecs.linea.LineaPro
  Get device information.
getInformation() - Method in class com.datecs.printer.Printer
  Returns the printer information.
getInformation(int) - Method in class com.datecs.printer.Printer
  Returns the printer information.
getInitialCapacity() - Method in class com.datecs.linea.LineaPro.BatteryInfo
  Get battery initial capacity in mAh.
getInputStream() - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Gets the input stream from channel.
getInternalTemperature() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get internal temperature in Kelvin (K).
getISO15424() - Method in class com.datecs.barcode.Barcode
  Get barcode type as ISO/IEC 15424.
getKeyInformation(int) - Method in class com.datecs.emsr.EMSR
  Returns information about keys into encrypted magnetic stripe reader (EMSR).
getLastError() - Method in class com.datecs.rfid.RFID
  Get last error.
getLibraryInformation() - Method in class com.datecs.biometric.TouchChip
  Return TouchChip library information.
getManufacturer() - Method in class com.datecs.linea.LineaProInformation
  Get device manufacturer.
getMaxLoadCurrent() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get max load current in mA.
getMaxPageHeight() - Method in class com.datecs.printer.PrinterInformation
  Returns maximum page height in dots.
getMaxPageWidth() - Method in class com.datecs.printer.PrinterInformation
  Returns maximum page width in dots.
getMifareReader() - Method in class com.datecs.universalreader.UniversalReader
  Returns an instance of `MifareReader` class.
getModel() - Method in class com.datecs.linea.LineaProInformation
  Get device model.
getModel() - Method in class com.datecs.printer.PrinterInformation
  Return printer model.
getModule() - Method in class com.datecs.rfid.ContactlessCard
  Get RFID for this card.
getName() - Method in class com.datecs.card.FinancialCard
  Returns a card holder's name of this financial card.
getName() - Method in class com.datecs.linea.LineaProInformation
  Get device name.
getName() - Method in class com.datecs.printer.PrinterInformation
  Returns printer name.
getNominalAvailableCapacity() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get nominal available capacity in mAh.
getNumber() - Method in class com.datecs.card.FinancialCard
  Returns a unique identifier of this financial card.
getNumberOfFingers() - Method in class com.datecs.biometric.AnsiIso
  Get number of finger/palm.
getOutputStream() - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Gets the input stream from channel.
getPixelDepth() - Method in class com.datecs.biometric.AnsiIso
  Get pixel depth.
getPressure() - Method in class com.datecs.universalreader.TouchEvent
  Gets the current pressure of this event.
getProductIdentifier() - Method in class com.datecs.biometric.AnsiIso
  Get product identifier.
getProductIdentifierAsHexString() - Method in class com.datecs.biometric.AnsiIso
  Get product identifier as HEX string.
getProtocol() - Method in class com.datecs.smartcard.AnswerToReset
  Returns a smart card communication protocol.
getRawInputStream() - Method in class com.datecs.printer.ProtocolAdapter
  Get input stream that is not wrap by protocol data.
getRawOutputStream() - Method in class com.datecs.printer.ProtocolAdapter
  Get output stream that is not wrap by protocol data.
getRecordLength() - Method in class com.datecs.biometric.AnsiIso
  Get record length.
getRemainingCapacity() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get remaining capacity in mAh.
getRTC() - Method in class com.datecs.linea.LineaPro
  Get real time clock.
getScaleUnits() - Method in class com.datecs.biometric.AnsiIso
  Get scale units.
getScanResolutionHorz() - Method in class com.datecs.biometric.AnsiIso
  Get scan resolution (horizontal).
getScanResolutionVert() - Method in class com.datecs.biometric.AnsiIso
  Get scan resolution (vertical).
getSerialNumber() - Method in class com.datecs.linea.LineaProInformation
  Get Device serial number.
getSerialNumber() - Method in class com.datecs.printer.Printer
  Return printer serial number.
getSerialNumber() - Method in class com.datecs.universalreader.UniversalReader
  Gets the device serial number.
getSerialNumber() - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Gets the serial number of Mifare reader.
getServiceCode() - Method in class com.datecs.card.FinancialCard
  Returns a service code.
getSettings(int) - Method in class com.datecs.printer.Printer
  Reading printer settings.
getSlaveState(int) - Method in class com.datecs.hub.Hub
  Get port state.
getSlaveType(int) - Method in class com.datecs.hub.Hub
  Get slave type.
getSlot() - Method in class com.datecs.biometric.TouchChip.Identity
  Get identity slot.
getSmartCardReader() - Method in class com.datecs.universalreader.UniversalReader
  Returns an instance of `SmartCardReader` class.
getStandbyCurrent() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get standby current in mA.
getState() - Method in class com.datecs.drawer.Drawer
  Get drawer state.
getStateOfCharge() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get state of charge in %.
getStateOfHealth() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get state of health in %.
getStatus() - Method in class com.datecs.printer.Printer
  Returns the printer status.
getStatus(int) - Method in class com.datecs.printer.Printer
  Returns the printer status.
getStatus() - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Gets status data from channel.
getStatus() - Method in class com.datecs.rfid.ISO14443Card.DESFire
getStatusCode() - Method in exception com.datecs.emsr.EMSRException
  Get status code that cause this exception.
getSW() - Method in class com.datecs.smartcard.ResponseAPDU
  Returns the value of the status bytes SW1 and SW2 as a single status word SW.
getSW1() - Method in class com.datecs.smartcard.ResponseAPDU
  Returns the value of the status byte SW1 as a value between 0 and 255.
getSW2() - Method in class com.datecs.smartcard.ResponseAPDU
  Returns the value of the status byte SW2 as a value between 0 and 255.
getTemperature() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get temperature in Kelvin (K).
getTemperature() - Method in class com.datecs.printer.Printer
  Returns the printer head temperature.
getTemplate(int) - Method in class com.datecs.biometric.TouchChip
  Get scanned template data.
getTemplate(int, int) - Method in class com.datecs.biometric.TouchChip
  Get template data from specific slot.
getTemplate(int, TouchChip.Template[]) - Method in class com.datecs.biometric.TouchChip
  Get scanned template data.
getTouchChip() - Method in class com.datecs.printer.Printer
  Get instance of TouchChip module.
getTouchScreen() - Method in class com.datecs.universalreader.UniversalReader
  Returns an instance of `Touchscreen` class.
getType() - Method in class com.datecs.barcode.Barcode
  Get barcode type.
getTypeName() - Method in class com.datecs.rfid.ContactlessCard
  Get card type name.
getTypeString() - Method in class com.datecs.barcode.Barcode
  Get barcode type as String.
getUID() - Method in class com.datecs.rfid.STSRICard
  Get UID.
getUsbDeviceDescriptor(int) - Method in class com.datecs.hub.Hub
  Get USB device descriptor.
getUsbStringDescriptor(int) - Method in class com.datecs.hub.Hub
  Get USB string descriptor.
getVersion() - Method in class com.datecs.linea.LineaProInformation
  Device firmware version.
getVersionNumber() - Method in class com.datecs.biometric.AnsiIso
  Get version number.
getVersionNumberAsString() - Method in class com.datecs.biometric.AnsiIso
  Get version number as String.
getVerticalLineLength() - Method in class com.datecs.biometric.AnsiIso
  Get vertical line length (image height).
getViewNumber() - Method in class com.datecs.biometric.AnsiIso
  Get view number.
getVoltage() - Method in class com.datecs.linea.LineaPro.BatteryInfo.Fuelgauge
  Get battery voltage level in mV.
getVoltage() - Method in class com.datecs.linea.LineaPro.BatteryInfo
  Get battery voltage level in mV.
getVoltage() - Method in class com.datecs.printer.Printer
  Returns the printer battery voltage.
getVoltagePercentage() - Method in class com.datecs.printer.Printer
  Returns the printer battery level in percents.
getX() - Method in class com.datecs.universalreader.TouchEvent
  Gets the X coordinate of this event.
getY() - Method in class com.datecs.universalreader.TouchEvent
  Gets the Y coordinate of this event.

## H

halt() - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Puts the selected Mifare card into 'idle' state.
hasBarcodeEngine() - Method in class com.datecs.linea.LineaProInformation
  Get if device has barcode engine.
hasEncryptedMagneticHead() - Method in class com.datecs.linea.LineaProInformation
  Get if device has encrypted magnetic head.
hasExternalSpeaker() - Method in class com.datecs.linea.LineaProInformation
  Get if device has external speaker.
hasIntermecEngine() - Method in class com.datecs.linea.LineaProInformation
  Get if device has Intermec barcode engine.
hasLED() - Method in class com.datecs.linea.LineaProInformation
  Get if device has LED panel.
hasMagneticHead() - Method in class com.datecs.linea.LineaProInformation
  Get if device has any magnetic head.
hasNewlandEngine() - Method in class com.datecs.linea.LineaProInformation
  Get if device has Newland barcode engine.
hasOpticodeEngine() - Method in class com.datecs.linea.LineaProInformation
  Get if device has Opticon barcode engine.
hasStandardMagneticHead() - Method in class com.datecs.linea.LineaProInformation
  Get if device has standard magnetic head.
HRI_ABOVE - Static variable in class com.datecs.printer.Printer
  The HRI code is drawn above the barcode.
HRI_BELOW - Static variable in class com.datecs.printer.Printer
  The HRI code is drawn below the barcode.
HRI_BOTH - Static variable in class com.datecs.printer.Printer
  The HRI code is drawn both above and below the barcode.
HRI_NONE - Static variable in class com.datecs.printer.Printer
  No HRI code is being drawn.
Hub - Class in com.datecs.hub
Hub(InputStream, OutputStream) - Constructor for class com.datecs.hub.Hub
  Constructs a new instance of this class from given InputStream and OutputStream.
Hub(FileDescriptor) - Constructor for class com.datecs.hub.Hub
  Constructs a new instance of this class from given FileDescriptor
HubException - Exception in com.datecs.hub
HubException(int) - Constructor for exception com.datecs.hub.HubException
hyatt64Card - Variable in class com.datecs.rfid.ContactlessCard
  The HYATT card enabled.

## I

IMAGE_COMPRESSION_NONE - Static variable in class com.datecs.biometric.TouchChip
  The image compression type.
IMAGE_COMPRESSION_WSQ - Static variable in class com.datecs.biometric.TouchChip
  WSQ compression type.
IMAGE_FORMAT_ANSI - Static variable in class com.datecs.biometric.TouchChip
  The image is in ANSI format.
IMAGE_FORMAT_ISO - Static variable in class com.datecs.biometric.TouchChip
  The image is in ISO format.
IMAGE_FORMAT_RAW - Static variable in class com.datecs.biometric.TouchChip
  The image is in RAW format.
IMAGE_SIZE_LARGE - Static variable in class com.datecs.biometric.TouchChip
  The image size is 256x360 pixels.
IMAGE_SIZE_SMALL - Static variable in class com.datecs.biometric.TouchChip
  The image size is 192x270 pixels.
increment(int, int, int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Performs value increment operation in Mifare card.
init(byte[]) - Method in class com.datecs.barcode.Intermec
init(byte[]) - Method in class com.datecs.barcode.Newland
initialize() - Method in class com.datecs.rfid.ContactlessCard
  Initialize card.
initialize() - Method in class com.datecs.rfid.FeliCaCard
  Initialize card.
initialize() - Method in class com.datecs.rfid.ISO14443Card
  Initialize card.
initialize() - Method in class com.datecs.rfid.ISO15693Card
  Initialize card.
initialize() - Method in class com.datecs.rfid.STSRICard
  Initialize card.
Intermec - Class in com.datecs.barcode
  Intermec barcode engine.
Intermec() - Constructor for class com.datecs.barcode.Intermec
Intermec.ProgressListener - Interface in com.datecs.barcode
IntermecBF4 - Class in com.datecs.barcode
IntermecBF4() - Constructor for class com.datecs.barcode.IntermecBF4
isBarcodeAvailable() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if barcode reader module is available.
isBatteryChargeEnabled() - Method in class com.datecs.linea.LineaPro
  Return whether mobile device battery charge is enabled.
isBlackmarkEnabled() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if blackmark mode is enabled.
isBlackmarkSupported() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if blackmark mode is supported.
isButtonPressed() - Method in class com.datecs.universalreader.UniversalReader
  Gets the current state of the button.
isButtonPressed(boolean) - Method in class com.datecs.universalreader.UniversalReader
  Gets the current state of the button.
isCardPresent() - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Returns if smart card is present into reader.
isCharging() - Method in class com.datecs.linea.LineaPro.BatteryInfo
  Get battery charging state.
isExternalSpeakerButtonEnabled() - Method in class com.datecs.linea.LineaPro
  Get whether external speaker button is enabled.
isExternalSpeakerEnabled() - Method in class com.datecs.linea.LineaPro
  Get whether external speaker is enabled.
isFahrenheit() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if head temperature is returned in Fahrenheit scale.
isFirmwareUpdateSupported() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if printer support firmware update.
isIrdaAvailable() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if IRDA module is available.
isMaxCurrentEnabled() - Method in class com.datecs.linea.LineaPro
  Get whether max current is enabled.
isMsr3Tack() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if magnetic stripe reader is capable to read track 3.
isMsrAvailable() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if magnetic stripe reader module is available.
ISO14443Card - Class in com.datecs.rfid
  A class that represents ISO14443 cards.
ISO14443Card(RC663) - Constructor for class com.datecs.rfid.ISO14443Card
  Constructs a new instance of this class.
ISO14443Card.DESFire - Class in com.datecs.rfid
ISO15693Card - Class in com.datecs.rfid
  A class that represents ISO15693 cards.
ISO15693Card(RC663) - Constructor for class com.datecs.rfid.ISO15693Card
  Constructs a new instance of this class.
isOpticonEngine() - Method in class com.datecs.barcode.Barcode
  Return if the barcode is scanned with opticon engine.
isPageSupported() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if page mode is supported.
isPresentB() - Method in class com.datecs.rfid.ISO14443Card
  Check if card present.
isProtocolEnabled() - Method in class com.datecs.printer.ProtocolAdapter
  Return `true` if protocol mode is currently enabled.
isScanButtonEnabled() - Method in class com.datecs.linea.LineaPro
  Return whether scan button is enabled.
isUsbAEnabled() - Method in class com.datecs.printer.PrinterInformation
  Return `true` if USB A is enabled.

## J

journalFormat() - Method in class com.datecs.printer.Printer
  Format journal
journalPrint() - Method in class com.datecs.printer.Printer
  Print journal
journalRead() - Method in class com.datecs.printer.Printer
  Read journal
journalRead(String) - Method in class com.datecs.printer.Printer
  Read journal
journalWrite(byte[]) - Method in class com.datecs.printer.Printer
  Write journal data.
journalWrite(String, String) - Method in class com.datecs.printer.Printer
  Write journal text.

## K

KEY_AES_AUTHENTICATION - Static variable in class com.datecs.emsr.EMSR
KEY_AES_DATA_ENCRYPTION - Static variable in class com.datecs.emsr.EMSR
  Encryption key, if set magnetic card data will be encrypted.
KEY_AES_KEK - Static variable in class com.datecs.emsr.EMSR
  Encrypted head key loading key.
KEY_DUKPT_MASTER - Static variable in class com.datecs.emsr.EMSR
  Encrypted head DUKPT master key.
KEY_NO_KEY - Static variable in class com.datecs.emsr.EMSR
  No key.
KEY_TMK_AES - Static variable in class com.datecs.emsr.EMSR
  Encrypted head TMK key.

## L

LineaPro - Class in com.datecs.linea
  This class implements support for LineaPro devices.
LineaPro(InputStream, OutputStream) - Constructor for class com.datecs.linea.LineaPro
  Constructs a new instance of this class from a given streams.
LineaPro.BarcodeListener - Interface in com.datecs.linea
  Interface definition for Barcode event callback.
LineaPro.BatteryInfo - Class in com.datecs.linea
  Battery information.
LineaPro.BatteryInfo.Fuelgauge - Class in com.datecs.linea
  Represents fuel gauge battery information.
LineaPro.ButtonListener - Interface in com.datecs.linea
  Interface definition for button event callback.
LineaPro.ConnectionListener - Interface in com.datecs.linea
  Interface definition for a Printer event callback.
LineaProException - Exception in com.datecs.linea
  Signals that an exception of some sort has occurred due execution of Linea Pro operation.
LineaProException(int) - Constructor for exception com.datecs.linea.LineaProException
  Initializes a new instance of the class with its error code.
LineaProInformation - Class in com.datecs.linea
  This class represents the various LineaPro device information.
listSlots() - Method in class com.datecs.biometric.TouchChip
  Lists all slots in which there is an enrolled template.
LOADER - Static variable in class com.datecs.barcode.IntermecBF4
loadKey(byte[]) - Method in class com.datecs.emsr.EMSR
  Loads new key, in plain or encrypted with already loaded AES256 Key Encryption Key (KEK).
loadKey(int, char, byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Store key in the internal module memory for later use.
loadKey(int, byte[]) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Stores key into Mifare reader EEPROM.
lockAFI() - Method in class com.datecs.rfid.ISO15693Card
  Locks ISO 15693 AFI preventing further changes.
lockBlock(int) - Method in class com.datecs.rfid.ISO15693Card
  Locks a single ISO 15693 card block.
lockDSFID() - Method in class com.datecs.rfid.ISO15693Card
  Locks ISO 15693 card DSFID preventing further changes.

## M

maxBlocks - Variable in class com.datecs.rfid.ContactlessCard
  The card max block size (Available for ISO15 cards only).
melody(String) - Method in class com.datecs.printer.Printer
  Making (beeping) a sequence of sounds with a certain frequency and duration.
mModule - Variable in class com.datecs.rfid.ContactlessCard
  The instance of RC663 module.
MODE_READ_JIS - Static variable in class com.datecs.emsr.EMSR
  Read JIS card.
MODE_READ_PREFIX - Static variable in class com.datecs.emsr.EMSR
  Read data with prefix before tracks - 0xF0, 0xF1, 0xF2.
MODE_READ_RAW - Static variable in class com.datecs.emsr.EMSR
  Read raw data.
MODE_READ_TRACK1 - Static variable in class com.datecs.emsr.EMSR
  Read track 1.
MODE_READ_TRACK2 - Static variable in class com.datecs.emsr.EMSR
  Read track 2.
MODE_READ_TRACK3 - Static variable in class com.datecs.emsr.EMSR
  Read track 3.

## N

NAME - Static variable in class com.datecs.BuildInfo
  The name of the product.
name - Variable in class com.datecs.emsr.EMSR.EMSRInformation
  Device representative name.
Newland - Class in com.datecs.barcode
Newland() - Constructor for class com.datecs.barcode.Newland

## O

obtainArray(byte[]) - Static method in class com.datecs.universalreader.TouchEvent
  Constructs a new instance of this class from a given byte array.
onBatteryStateChanged(boolean) - Method in interface com.datecs.printer.ProtocolAdapter.PrinterListener
  This method is invoke when printer battery state is changed.
onButtonStateChanged(int, boolean) - Method in interface com.datecs.linea.LineaPro.ButtonListener
  This method is called when states of button is changed.
OnButtonStateChanged(boolean) - Method in interface com.datecs.universalreader.UniversalReader.ButtonListener
  This method is invoke when button state is changed.
onCardDetect(ContactlessCard) - Method in interface com.datecs.rfid.RC663.CardListener
onDataReceived(int, int, byte[]) - Method in interface com.datecs.biometric.TouchChip.ImageReceiver
  Invokes when new data is received.
onDataReceived(byte[], int) - Method in class com.datecs.rfid.RC663
onDataReceived(byte[], int) - Method in class com.datecs.rfid.RFID
  Abstract method that is called when data is received.
onDisconnect() - Method in interface com.datecs.drawer.Drawer.ConnectionListener
  This method is called when device connection is closed.
onDisconnect() - Method in interface com.datecs.linea.LineaPro.ConnectionListener
  This method is called when LineaPro connection is closed.
onDisconnect() - Method in interface com.datecs.printer.Printer.ConnectionListener
  This method is called when Printer connection is closed.
onDisconnect() - Method in interface com.datecs.universalreader.UniversalReader.ConnectionListener
  This method is called when Printer connection is closed.
onPaperStateChanged(boolean) - Method in interface com.datecs.printer.ProtocolAdapter.PrinterListener
  This method is invoke when paper state is changes.
onProgressUpdate(String, int) - Method in interface com.datecs.barcode.Intermec.ProgressListener
onReadBarcode(Barcode) - Method in interface com.datecs.linea.LineaPro.BarcodeListener
  This method is called when Barcode data is available.
onReadBarcode() - Method in interface com.datecs.printer.ProtocolAdapter.BarcodeListener
  This method is invoke when barcode is read.
onReadBarcode(int, byte[]) - Method in interface com.datecs.universalreader.UniversalReader.BarcodeListener
  This method is invoke when barcode is read.
onReadCard(boolean) - Method in interface com.datecs.printer.ProtocolAdapter.CardListener
  This method is invoke when magnetic card is read.
onReadCard(boolean) - Method in interface com.datecs.universalreader.UniversalReader.CardListener
  This method is invoke when magnetic card is read.
onSlaveConnected(int) - Method in interface com.datecs.hub.SlaveConnection
  This method is called when new device is connected.
onSlaveDisconnected(int, boolean) - Method in interface com.datecs.hub.SlaveConnection
  This method is call when device is disconnected or communication is not possible.
onStateChanged(boolean) - Method in interface com.datecs.drawer.Drawer.StateListener
  This method is called when device state is changed.
onThermalHeadStateChanged(boolean) - Method in interface com.datecs.printer.ProtocolAdapter.PrinterListener
  This method is invoke when printer thermal head state is changed.
open(int) - Method in class com.datecs.drawer.Drawer
  Open drawer with specified impulse.
open() - Method in class com.datecs.drawer.Drawer
  Open drawer with default impulse (30).
open() - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Open channel.

## P

PAGE_BOTTOM - Static variable in class com.datecs.printer.Printer
  Printing from bottom to top, feed to right.
PAGE_LEFT - Static variable in class com.datecs.printer.Printer
  Printing page from left to right, feed to bottom.
PAGE_RIGHT - Static variable in class com.datecs.printer.Printer
  Printing page from right to left, feed to top.
PAGE_TOP - Static variable in class com.datecs.printer.Printer
  Printing page from top to bottom, feed to left.
parse(byte[]) - Static method in class com.datecs.barcode.Barcode
  Parse data to return barcode information.
playSound(int, int) - Method in class com.datecs.universalreader.UniversalReader
  Plays sound via device buzzer.
printArabicText(int, String) - Method in class com.datecs.printer.Printer
  Print Arabic text.
printBarcode(int, byte[]) - Method in class com.datecs.printer.Printer
  Prints a barcode.
printBarcode(int, String) - Method in class com.datecs.printer.Printer
  Prints a barcode.
printCompressedImage(int[], int, int, int, boolean, boolean) - Method in class com.datecs.printer.Printer
printCompressedImage(int[], int, int, int, boolean) - Method in class com.datecs.printer.Printer
Printer - Class in com.datecs.printer
  This class implements support for Datecs's ESC/P printers.
Printer(OutputStream) - Constructor for class com.datecs.printer.Printer
  Constructs a new instance of this class from a given `OutputStream`.
Printer(InputStream, OutputStream) - Constructor for class com.datecs.printer.Printer
  Constructs a new instance of this class from a given `InputStream` and `OutputStream`.
Printer.ConnectionListener - Interface in com.datecs.printer
  Interface definition for a Printer event callback.
PRINTER_CMP10 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_DPP250 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_DPP350 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_DPP450 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_DPP500 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_EP300 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_EP55 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_EP60 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_PP60 - Static variable in class com.datecs.printer.PrinterInformation
PRINTER_UNKNOWN - Static variable in class com.datecs.printer.PrinterInformation
PrinterInformation - Class in com.datecs.printer
  This class represents a various information received from printer.
printImage(int[], int, int, int, boolean, boolean) - Method in class com.datecs.printer.Printer
printImage(int[], int, int, int, boolean) - Method in class com.datecs.printer.Printer
printLogo(boolean, boolean) - Method in class com.datecs.printer.Printer
  Prints a stored bit image (logo).
printLogo() - Method in class com.datecs.printer.Printer
  Prints a stored bit image (logo).
printPage() - Method in class com.datecs.printer.Printer
  Prints the non blank page area only in page mode.
printQRCode(int, int, byte[]) - Method in class com.datecs.printer.Printer
  Prints the QRCode.
printQRCode(int, int, String) - Method in class com.datecs.printer.Printer
  Prints the QRCode.
printSelfTest() - Method in class com.datecs.printer.Printer
  Prints self test receipt.
printTaggedText(String) - Method in class com.datecs.printer.Printer
  Prints a tagged text using default charset for encoding.
printTaggedText(String, String) - Method in class com.datecs.printer.Printer
  Prints a tagged text using the named charset for encoding.
printText(byte[]) - Method in class com.datecs.printer.Printer
  Prints a text using default charset for encoding.
printText(String) - Method in class com.datecs.printer.Printer
  Prints a text using default charset for encoding.
printText(String, String) - Method in class com.datecs.printer.Printer
  Prints a text using the named charset for encoding.
PROTOCOL_T0 - Static variable in class com.datecs.smartcard.AnswerToReset
  ISO/IEC 7816-4 transport protocol type T=0.
PROTOCOL_T1 - Static variable in class com.datecs.smartcard.AnswerToReset
  ISO/IEC 7816-4 transport protocol type T=1.
ProtocolAdapter - Class in com.datecs.printer
  This class provides the protocol mode support for Datecs's printers over InputStream and OutputStream instances.
ProtocolAdapter(InputStream, OutputStream) - Constructor for class com.datecs.printer.ProtocolAdapter
  Constructs a new instance of this class from a given `InputStream` and `OutputStream`.
ProtocolAdapter.BarcodeListener - Interface in com.datecs.printer
  Interface definition for a callbacks to notify for barcode event.
ProtocolAdapter.CardListener - Interface in com.datecs.printer
  Interface definition for a callbacks to notify for card event.
ProtocolAdapter.Channel - Class in com.datecs.printer
  This class represents a protocol channel.
ProtocolAdapter.PrinterListener - Interface in com.datecs.printer
  Interface definition for a callbacks to notify for printer event.

## Q

query(byte[]) - Method in class com.datecs.barcode.Intermec

## R

RC663 - Class in com.datecs.rfid
  This class represents RC663 module.
RC663(InputStream, OutputStream, int) - Constructor for class com.datecs.rfid.RC663
  Constructs a new instance of this class.
RC663(InputStream, OutputStream) - Constructor for class com.datecs.rfid.RC663
  Constructs a new instance of this class.
RC663.CardListener - Interface in com.datecs.rfid
read() - Method in class com.datecs.barcode.Intermec
read(int, int, int) - Method in class com.datecs.rfid.FeliCaCard
  Reads one more more blocks of data from FeliCa card.
read(int, int) - Method in class com.datecs.rfid.ISO15693Card
  Reads one more more blocks of data from ISO 15693 card.
read() - Method in class com.datecs.universalreader.UniversalReader.BarcodeReader
  Reads barcode.
read(int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Reads block from Mifare card.
read(int, int, int, int, int) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Sends APDU read request.
read(byte[]) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Sends APDU read request.
read16(int) - Method in class com.datecs.rfid.ISO14443Card
  Reads one block of data from Mifare Classic/Ultralight cards.
readBarcode(int) - Method in class com.datecs.printer.Printer
  Reads the barcode.
readBlock(int) - Method in class com.datecs.rfid.STSRICard
  Reads one more more blocks of data from ST SRI card.
readCard(boolean, boolean, boolean, int) - Method in class com.datecs.printer.Printer
  Reads the magnetic stripe card.
readCardData(int) - Method in class com.datecs.emsr.EMSR
  Read card data.
readEeprom(int, int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Reads data from Mifare reader EEPROM memory.
readFile(int, int) - Method in class com.datecs.rfid.ISO14443Card.DESFire
readNVRAM(int) - Method in class com.datecs.hub.Hub
  Read data from NV memory.
readTrackData(int) - Method in class com.datecs.universalreader.UniversalReader
  Read track data.
request(boolean) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Requests for Mifare cards.
reset() - Method in class com.datecs.printer.Printer
  Resets printer to it's default settings.
reset() - Method in class com.datecs.rfid.STSRICard
  Card reset.
reset() - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Resets the smart card and returns the ATR.
ResponseAPDU - Class in com.datecs.smartcard
  This class represents the smart card response APDU as defined in ISO/IEC 7816-4.
ResponseAPDU(byte[]) - Constructor for class com.datecs.smartcard.ResponseAPDU
  Constructs a new instance of this class from a given byte array containing the complete APDU contents.
restore(int, int, int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Performs value restore operation in Mifare card.
resume() - Method in class com.datecs.printer.ProtocolAdapter.Channel
resume() - Method in class com.datecs.rfid.RC663
  Reinitialize RF card reader module to listen for cards.
RFID - Class in com.datecs.rfid
  Class that represents RFID module.
RFID_MODULE_CLRC663 - Static variable in class com.datecs.linea.LineaPro
  CLRC663 RFID chip.
RFID_MODULE_MURATA - Static variable in class com.datecs.linea.LineaPro
  MURATA RFID chip.
RFIDException - Exception in com.datecs.rfid
  The exception that is thrown when an RC663 module error occurs.
RFIDException(int) - Constructor for exception com.datecs.rfid.RFIDException
  Initializes a new instance of the RC663Exception class with its error code.
rfidGetModule() - Method in class com.datecs.linea.LineaPro
  Returns instance to RFID module
rfidTransmit(int, byte[]) - Method in class com.datecs.linea.LineaPro
  Transmit data to RFID module.
RSA - Class in com.datecs.crypto
  Helper methods to encrypt or decrypt with RSA algorithm.
RSA() - Constructor for class com.datecs.crypto.RSA

## S

sak - Variable in class com.datecs.rfid.ContactlessCard
  The card SAK (Available for MIFARE cards only).
saveSettings() - Method in class com.datecs.linea.LineaPro
  Force save settings.
saveSymbology() - Method in class com.datecs.barcode.Intermec
  Store barcode settings in barcode flash memory.
select(int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Selects a Mifare card.
select(int) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Selects the smart card reader slot.
selectApplication(int) - Method in class com.datecs.rfid.ISO14443Card.DESFire
selectCodetable(int) - Method in class com.datecs.printer.Printer
  Selects a code table.
selectPageMode() - Method in class com.datecs.printer.Printer
  Switches from standard mode to page mode.
selectStandardMode() - Method in class com.datecs.printer.Printer
  Switches from page mode to standard mode.
sendCommand(byte[]) - Method in class com.datecs.barcode.Intermec
  Send command to barcode engine.
serial - Variable in class com.datecs.emsr.EMSR.EMSRInformation
  Device serial number
setAlign(int) - Method in class com.datecs.printer.Printer
  Sets alignment for the next printed text row or object.
setAppleChargeCurrent(int) - Method in class com.datecs.hub.Hub
  Set Apple devices charge current.
setAutoOff(int) - Method in class com.datecs.universalreader.UniversalReader
  Set auto off time.
setAutoOffTime(boolean, int) - Method in class com.datecs.linea.LineaPro
  Set the time after which the device shall automatically goes off.
setBarcode(int, boolean, int, int, int) - Method in class com.datecs.printer.Printer
  Sets the various barcode parameters.
setBarcodeListener(LineaPro.BarcodeListener) - Method in class com.datecs.linea.LineaPro
  Set on barcode listener.
setBarcodeListener(ProtocolAdapter.BarcodeListener) - Method in class com.datecs.printer.ProtocolAdapter
  Set a callback listener to notify for barcode event.
setBarcodeListener(UniversalReader.BarcodeListener) - Method in class com.datecs.universalreader.UniversalReader
  Set a callback listener to notify for barcode event.
setBaudRate(int, int) - Method in class com.datecs.hub.Hub
  Set RS232 baud rate.
setButton(int) - Method in class com.datecs.universalreader.UniversalReader
  Set button function mode
setButtonListener(LineaPro.ButtonListener) - Method in class com.datecs.linea.LineaPro
  Set button switch listener.
setButtonListener(UniversalReader.ButtonListener) - Method in class com.datecs.universalreader.UniversalReader
  Set a callback listener to notify for button state changed.
setCardListener(ProtocolAdapter.CardListener) - Method in class com.datecs.printer.ProtocolAdapter
  Set a callback listener to notify for card event.
setCardListener(RC663.CardListener) - Method in class com.datecs.rfid.RC663
  Set a callback to notify when new card available.
setCardListener(UniversalReader.CardListener) - Method in class com.datecs.universalreader.UniversalReader
  Set a callback listener to notify for card event.
setChannel(int, int) - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Sets channel associated port.
setConnectionListener(Drawer.ConnectionListener) - Method in class com.datecs.drawer.Drawer
  Set a callback listener to notify the connection state is changed.
setConnectionListener(LineaPro.ConnectionListener) - Method in class com.datecs.linea.LineaPro
  Set a callback listener to notify the connection state is changed.
setConnectionListener(Printer.ConnectionListener) - Method in class com.datecs.printer.Printer
  Set a callback listener to notify the connection state is changed.
setConnectionListener(UniversalReader.ConnectionListener) - Method in class com.datecs.universalreader.UniversalReader
  Set a callback listener to notify the connection state is changed.
setDebug(boolean) - Static method in class com.datecs.drawer.Drawer
  Turn on/off debugging.
setDebug(boolean) - Static method in class com.datecs.emsr.EMSR
  Specify whether the object can output debug information
setDebug(boolean) - Static method in class com.datecs.hub.Hub
  Enable or disable debug output.
setDebug(boolean) - Static method in class com.datecs.linea.LineaPro
  Turn on/off debugging.
setDebug(boolean) - Static method in class com.datecs.printer.Printer
  Specify whether the object can output debug information
setDebug(boolean) - Static method in class com.datecs.printer.ProtocolAdapter
  Specify whether the object can output debug information
setDebug(boolean) - Static method in class com.datecs.rfid.RFID
  Turn on/off debugging.
setDebug(boolean) - Static method in class com.datecs.universalreader.UniversalReader
  Specify whether the object can output debug information
setDeviceMode(int) - Method in class com.datecs.linea.LineaPro
  Set the device mode.
setEncryptionType(int) - Method in class com.datecs.emsr.EMSR
  Set encryption type.
setIlluminationLevel(int) - Method in class com.datecs.barcode.Intermec
  Set illumination level
setIntensity(int) - Method in class com.datecs.printer.Printer
  Set intensity level.
setLED(boolean, boolean, boolean) - Method in class com.datecs.linea.LineaPro
  Turn on the LEDs.
setLedMode(int) - Method in class com.datecs.printer.ProtocolAdapter.Channel
  Set LED indicator mode.
setLineSpace(int) - Method in class com.datecs.printer.Printer
  Sets the line space of text rows.
setPageRegion(int, int, int, int, int) - Method in class com.datecs.printer.Printer
  Defines the relative position, size print direction of the page.
setPageXY(int, int) - Method in class com.datecs.printer.Printer
  Sets the print position in current page region.
setPollingParams(int, int, int, int, int) - Method in class com.datecs.rfid.RC663
  Set polling parameter for FeliCa Card
setPower(boolean) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Powers on/off Mifare card reader.
setPower(boolean) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Powers on/off smart card.
setPredefinedImagerSettings(int) - Method in class com.datecs.barcode.Intermec
  Set pre-defined imager settings.
setPresenterActiveMode(int) - Method in class com.datecs.printer.Printer
  Select the active mode on the presenter.
setPresenterOpMode(int) - Method in class com.datecs.printer.Printer
  Select the presenter operation.
setPrinterListener(ProtocolAdapter.PrinterListener) - Method in class com.datecs.printer.ProtocolAdapter
  Set a callback listener to notify for printer event.
setQRCode(int) - Method in class com.datecs.printer.Printer
  Sets the cell size for two dimensional barcode QR Code.
setRetractiveModeTimeout(int) - Method in class com.datecs.printer.Printer
  Set the time-out for the retractive mode.
setRTC(Calendar) - Method in class com.datecs.linea.LineaPro
  Set real time clock.
setSlaveConnectionListener(SlaveConnection) - Method in class com.datecs.hub.Hub
  Set slave connection listener.
setStateListener(Drawer.StateListener) - Method in class com.datecs.drawer.Drawer
  Set a callback listener to notify when device state is changed.
setTemplate(int, byte[]) - Method in class com.datecs.biometric.TouchChip
  Set template data to into TouchChip module non-volatile memory.
SETTINGS_BLUETOOTH - Static variable in class com.datecs.printer.Printer
  Bluetooth settings.
SHA1 - Class in com.datecs.crypto
  SHA1
SHA1() - Constructor for class com.datecs.crypto.SHA1
SHA256 - Class in com.datecs.crypto
  SHA256
SHA256() - Constructor for class com.datecs.crypto.SHA256
signSHA256(byte[], byte[], byte[]) - Static method in class com.datecs.crypto.RSA
  Sign SHA256 with RSA.
SLAVE_STATE_DISCONNECTED - Static variable in class com.datecs.hub.Hub
  Slave is disconnected.
SLAVE_STATE_ERROR - Static variable in class com.datecs.hub.Hub
  Slave error state (i.e.
SLAVE_STATE_READY - Static variable in class com.datecs.hub.Hub
  Slave is ready.
SLAVE_STATE_UNKNOWN - Static variable in class com.datecs.hub.Hub
  Slave state is unknown.
SLAVE_TYPE_RS232 - Static variable in class com.datecs.hub.Hub
  RS232 slave type.
SLAVE_TYPE_USB - Static variable in class com.datecs.hub.Hub
  USB slave type.
SlaveConnection - Interface in com.datecs.hub
  Listen for slave connection state changed.
smartTagClearScreen() - Method in class com.datecs.rfid.FeliCaCard
  Clears the screen of FeliCa SmartTag.
smartTagDisplayLayout(int) - Method in class com.datecs.rfid.FeliCaCard
  Displays previously stored layout.
smartTagDrawImage(int, int, int, int, int, int, byte[]) - Method in class com.datecs.rfid.FeliCaCard
  Draws image on FeliCa SmartTag's screen.
smartTagGetBatteryStatus() - Method in class com.datecs.rfid.FeliCaCard
  Returns FeliCa SmartTag battery status.
smartTagRead(int, int) - Method in class com.datecs.rfid.FeliCaCard
  Writes data in FeliCa SmartTag.
smartTagSaveLayout(int) - Method in class com.datecs.rfid.FeliCaCard
  Saves the current display as layout number.
smartTagWrite(int, byte[]) - Method in class com.datecs.rfid.FeliCaCard
  Writes data in FeliCa SmartTag.
startVibrator(int) - Method in class com.datecs.linea.LineaPro
  Turn on the vibrator for a specified time.
STATUS_EMSR_BAD_ARRAY - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_BARCODE_MISHMASH - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_BARCODE_NO_READER - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_CARD_ERROR - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_HARD - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_INVALID_COMMAND - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_INVALID_LENGTH - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_INVALID_SIGNATURE - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_NO_BARCODE_READ - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_NO_DATA - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_NO_PERMISSION - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_NO_RESPONSE - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_SYNTAX_ERROR - Static variable in class com.datecs.emsr.EMSR
STATUS_EMSR_TAMPERED - Static variable in class com.datecs.emsr.EMSR
STSRICard - Class in com.datecs.rfid
STSRICard(RC663) - Constructor for class com.datecs.rfid.STSRICard
  Constructs a new instance of this class.
suspend() - Method in class com.datecs.printer.ProtocolAdapter.Channel

## T

tampered - Variable in class com.datecs.emsr.EMSR.EMSRKeyInformation
  Shows if devices is tampered.
Template(int, byte[]) - Constructor for class com.datecs.biometric.TouchChip.Template
TEMPLATE_FORMAT_ANSI - Static variable in class com.datecs.biometric.TouchChip
  Template in ANSI (ANSI INCITS 378-2004) format.
TEMPLATE_FORMAT_ISO_FMC_C - Static variable in class com.datecs.biometric.TouchChip
  Template in ISO_FMC_C (ISO/IEC 19794-2-2005) card format.
TEMPLATE_FORMAT_ISO_FMC_N - Static variable in class com.datecs.biometric.TouchChip
  Template in ISO_FMC_N (ISO/IEC 19794-2-2005) card format.
TEMPLATE_FORMAT_ISO_FMR - Static variable in class com.datecs.biometric.TouchChip
  Template in ISO_FMR (ISO/IEC 19794-2-2005) format
TEMPLATE_FORMAT_NATIVE - Static variable in class com.datecs.biometric.TouchChip
  Template in NATIVE (AuthenTec legacy) format.
test(int) - Method in class com.datecs.emsr.EMSR
  Test encrypted magnetic head.
toString() - Method in class com.datecs.barcode.Barcode
toString() - Method in class com.datecs.biometric.AnsiIso
toString() - Method in class com.datecs.biometric.TouchChip.Identity
toString() - Method in class com.datecs.card.FinancialCard
  Returns the string representation of object.
toString() - Method in class com.datecs.emsr.EMSR.EMSRInformation
toString() - Method in class com.datecs.emsr.EMSR.EMSRKeyInformation
toString() - Method in exception com.datecs.linea.LineaProException
toString() - Method in class com.datecs.smartcard.AnswerToReset
  Returns the string representation of object.
toString() - Method in class com.datecs.smartcard.ResponseAPDU
  Returns the string representation of object.
toString() - Method in class com.datecs.universalreader.TouchEvent
  Returns the string representation of object.
TouchChip - Class in com.datecs.biometric
  Implements functionality of TouchChip finger print module.
TouchChip() - Constructor for class com.datecs.biometric.TouchChip
  Constructs a new instance of this class.
TouchChip.Identity - Class in com.datecs.biometric
  The class that contains identity information.
TouchChip.ImageReceiver - Interface in com.datecs.biometric
  A callback interface to notify when image data is received.
TouchChip.Template - Class in com.datecs.biometric
TouchChipException - Exception in com.datecs.biometric
  Signals that an exception of some sort has occurred due execution of TouchChip operation.
TouchChipException() - Constructor for exception com.datecs.biometric.TouchChipException
  Constructs a new instance of this class.
TouchChipException(String) - Constructor for exception com.datecs.biometric.TouchChipException
  Constructs a new instance of this class.
TouchChipException(int) - Constructor for exception com.datecs.biometric.TouchChipException
  Constructs a fully-specified instance of this class.
TouchEvent - Class in com.datecs.universalreader
  This class is used to report single touch event from touch screen peripherals.
TouchEvent(int, int, int, int) - Constructor for class com.datecs.universalreader.TouchEvent
  Constructs a `TouchEvent`, filling in all of the basic values that define the touch.
TR31 - Class in com.datecs.crypto
TR31() - Constructor for class com.datecs.crypto.TR31
transceive(byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Transceive data to ISO14443
transceiveA(byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Transceive data to ISO14443 A
transceiveB(byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Transceive data to ISO14443 B
transmit(byte[]) - Method in class com.datecs.biometric.TouchChip
  Transmit packet to module.
transmit(int, int, int, int, byte[]) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Sends combined APDU write/read request.
transmit(byte[]) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Sends combined APDU write/read request.
transmit(List<byte[]>) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Sends list of combined APDU write/read requests.
transmitCard(int, byte[]) - Method in class com.datecs.rfid.RC663
  Transmit command data to card.
transmitCard(int, byte[], int) - Method in class com.datecs.rfid.RC663
  Transmit command data to card.
transmitEMSR(byte[]) - Method in class com.datecs.emsr.EMSR
  Transmit data to encrypted magnetic stripe reader (EMSR).
TripleDES - Class in com.datecs.crypto
  Helper methods to encrypt or decrypt with Triple DES algorithm.
TripleDES() - Constructor for class com.datecs.crypto.TripleDES
turnOff() - Method in class com.datecs.linea.LineaPro
  Turn off the device.
turnOff() - Method in class com.datecs.printer.Printer
  Turn off printer.
turnOff() - Method in class com.datecs.universalreader.UniversalReader
  Turn off the device.
turnOffScopeScaling() - Method in class com.datecs.barcode.Newland
turnOnScopeScaling(int) - Method in class com.datecs.barcode.Newland
type - Variable in class com.datecs.rfid.ContactlessCard
  The card type.

## U

uid - Variable in class com.datecs.rfid.ContactlessCard
  The card UID.
ulcAuthenticate(byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Performs 3DES authentication of Mifare Ultralight C card using the given key.
ulcSetKey(byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Sets the 3DES key of Mifare Ultralight C cards.
UniversalReader - Class in com.datecs.universalreader
  This class provides functionality for CAC2, PDA+, SCP10, PP-55 Smart Card Reader, PP-55/DPP-250/DPP-350 Universal Readers and any other device that supports Universal Reader protocol.
UniversalReader(InputStream, OutputStream) - Constructor for class com.datecs.universalreader.UniversalReader
  Constructs a new instance of this class from a given `InputStream` and `OutputStream`.
UniversalReader.BarcodeListener - Interface in com.datecs.universalreader
  Interface definition for a callbacks to notify for barcode event.
UniversalReader.BarcodeReader - Class in com.datecs.universalreader
  This class provides functionality for Barcode reader.
UniversalReader.ButtonListener - Interface in com.datecs.universalreader
  Interface definition for a callbacks to notify for button event.
UniversalReader.CardListener - Interface in com.datecs.universalreader
  Interface definition for a callbacks to notify for card event.
UniversalReader.ConnectionListener - Interface in com.datecs.universalreader
  Interface definition for a Printer event callback.
UniversalReader.MifareReader - Class in com.datecs.universalreader
  This class provides functionality for the Mifare reader.
UniversalReader.SmartCardReader - Class in com.datecs.universalreader
  This class provides functionality for the Smart Card reader.
UniversalReader.TouchScreen - Class in com.datecs.universalreader
  This class provides functionality for the Touchscreen.
UniversalReaderException - Exception in com.datecs.universalreader
  Signals that an exception of some sort has occurred due execution of Universal Reader operation.
UniversalReaderException() - Constructor for exception com.datecs.universalreader.UniversalReaderException
  Constructs a new instance of this class.
UniversalReaderException(String) - Constructor for exception com.datecs.universalreader.UniversalReaderException
  Constructs a new instance of this class.
UniversalReaderException(int) - Constructor for exception com.datecs.universalreader.UniversalReaderException
  Constructs a fully-specified instance of this class.
updateFirmware(byte[], Intermec.ProgressListener) - Method in class com.datecs.barcode.Intermec
updateMode(byte[]) - Method in class com.datecs.barcode.Intermec

## V

valueOf(String) - Static method in enum com.datecs.crypto.DUKPT.DerivationPurpose
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.datecs.crypto.DUKPT.KeyType
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.datecs.crypto.DUKPT.KeyUsage
  Returns the enum constant of this type with the specified name.
values() - Static method in enum com.datecs.crypto.DUKPT.DerivationPurpose
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.datecs.crypto.DUKPT.KeyType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.datecs.crypto.DUKPT.KeyUsage
  Returns an array containing the constants of this enum type, in the order they are declared.
verify(byte[], byte[], int, int) - Static method in class com.datecs.crypto.SHA1
verify(byte[], byte[], int, int) - Static method in class com.datecs.crypto.SHA256
VERSION - Static variable in class com.datecs.BuildInfo
  The user-visible version string.
version - Variable in class com.datecs.emsr.EMSR.EMSRInformation
  Device firmware version.
version - Variable in class com.datecs.emsr.EMSR.EMSRKeyInformation
  Key version.

## W

waitRemove() - Method in class com.datecs.rfid.ContactlessCard
  Call this function once you are done with the card.
wipeIdentity() - Method in class com.datecs.biometric.TouchChip
  Wipe identity content.
write(byte[]) - Method in class com.datecs.barcode.Intermec
write(int) - Method in class com.datecs.printer.Printer
  Writes the specified byte to this printer.
write(byte[]) - Method in class com.datecs.printer.Printer
  Writes all bytes from the specified byte array to this printer.
write(byte[], int, int) - Method in class com.datecs.printer.Printer
  Writes `length` bytes from the specified byte array to this printer.
write(int, int, byte[]) - Method in class com.datecs.rfid.FeliCaCard
  Writes one more more blocks of data to FeliCa card.
write(int, byte[]) - Method in class com.datecs.rfid.ISO15693Card
  Writes one more more blocks of data to ISO 15693 card.
write(int, byte[]) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Writes block to Mifare card.
write(int, int) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Writes data to Mifare card.
write(int, int, int, int, byte[]) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Sends APDU write request.
write(byte[]) - Method in class com.datecs.universalreader.UniversalReader.SmartCardReader
  Sends APDU write request.
write16(int, byte[]) - Method in class com.datecs.rfid.ISO14443Card
  Writes one block of data to Mifare Classic/Ultralight cards.
write4(int, byte[]) - Method in class com.datecs.rfid.ISO14443Card
writeAFI(byte) - Method in class com.datecs.rfid.ISO15693Card
  Changes ISO 15693 card AFI.
writeBlock(byte[], int, int) - Method in class com.datecs.rfid.RFID
  Writes length bytes from the specified byte array to this printer.
writeBlock(int, byte[]) - Method in class com.datecs.rfid.STSRICard
  Writes one more more blocks of data to ST SRI card.
writeDSFID(byte) - Method in class com.datecs.rfid.ISO15693Card
  Changes ISO 15693 card DSFID.
writeEeprom(int, byte[]) - Method in class com.datecs.universalreader.UniversalReader.MifareReader
  Writes data to Mifare reader EEPROM memory.
writeFile(int, byte[]) - Method in class com.datecs.rfid.ISO14443Card.DESFire
writeNVRAM(int, byte[]) - Method in class com.datecs.hub.Hub
  Write data to NV memory.

A B C D E F G H I J K L M N O P Q R S T U V W