# Constant Field Values

## Contents

- com.datecs.*

## com.datecs.*

- com.datecs.BuildInfo
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `BUILD_DATE` | `"20200929130430"`
  `public static final java.lang.String` | `NAME` | `"lib"`
  `public static final java.lang.String` | `VERSION` | `"4.3.35"`

- com.datecs.barcode.Barcode
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `BARCODE_ALL` | `0`
  `public static final int` | `BARCODE_AZTEK` | `31`
  `public static final int` | `BARCODE_CCA` | `56`
  `public static final int` | `BARCODE_CCB` | `57`
  `public static final int` | `BARCODE_CCC` | `58`
  `public static final int` | `BARCODE_CODABAR` | `2`
  `public static final int` | `BARCODE_CODABAR_ABC` | `50`
  `public static final int` | `BARCODE_CODABAR_CX` | `51`
  `public static final int` | `BARCODE_CODE11` | `8`
  `public static final int` | `BARCODE_CODE128` | `7`
  `public static final int` | `BARCODE_CODE25_I2OF5` | `4`
  `public static final int` | `BARCODE_CODE25_NI2OF5` | `3`
  `public static final int` | `BARCODE_CODE39` | `5`
  `public static final int` | `BARCODE_CODE39_FULL` | `48`
  `public static final int` | `BARCODE_CODE93` | `6`
  `public static final int` | `BARCODE_CPCBINARY` | `9`
  `public static final int` | `BARCODE_DATAMATRIX` | `30`
  `public static final int` | `BARCODE_DUN14` | `10`
  `public static final int` | `BARCODE_EAN128` | `15`
  `public static final int` | `BARCODE_EAN13` | `14`
  `public static final int` | `BARCODE_EAN13_2` | `44`
  `public static final int` | `BARCODE_EAN13_5` | `45`
  `public static final int` | `BARCODE_EAN2` | `11`
  `public static final int` | `BARCODE_EAN5` | `12`
  `public static final int` | `BARCODE_EAN8` | `13`
  `public static final int` | `BARCODE_EAN8_2` | `46`
  `public static final int` | `BARCODE_EAN8_5` | `47`
  `public static final int` | `BARCODE_GS1DATABAR` | `16`
  `public static final int` | `BARCODE_IATA` | `54`
  `public static final int` | `BARCODE_INTELLIGENT_MAIL` | `22`
  `public static final int` | `BARCODE_ITA_PHARMA` | `49`
  `public static final int` | `BARCODE_ITF14` | `17`
  `public static final int` | `BARCODE_KOREAN_POSTAL` | `55`
  `public static final int` | `BARCODE_LAST` | `59`
  `public static final int` | `BARCODE_LATENT_IMAGE` | `18`
  `public static final int` | `BARCODE_MATRIX_2OF5` | `53`
  `public static final int` | `BARCODE_MAXICODE` | `33`
  `public static final int` | `BARCODE_MICROPDF417` | `29`
  `public static final int` | `BARCODE_MSI_PLESSEY` | `23`
  `public static final int` | `BARCODE_PDF417` | `28`
  `public static final int` | `BARCODE_PHARMACODE` | `19`
  `public static final int` | `BARCODE_PLANET` | `20`
  `public static final int` | `BARCODE_POSTBAR` | `24`
  `public static final int` | `BARCODE_POSTNET` | `21`
  `public static final int` | `BARCODE_QRCODE` | `32`
  `public static final int` | `BARCODE_RESERVED1` | `34`
  `public static final int` | `BARCODE_RESERVED2` | `35`
  `public static final int` | `BARCODE_RESERVED3` | `36`
  `public static final int` | `BARCODE_RESERVED4` | `37`
  `public static final int` | `BARCODE_RESERVED5` | `38`
  `public static final int` | `BARCODE_RM4SCC` | `25`
  `public static final int` | `BARCODE_SCODE` | `52`
  `public static final int` | `BARCODE_TELEPEN` | `26`
  `public static final int` | `BARCODE_UK_PLESSEY` | `27`
  `public static final int` | `BARCODE_UNKNOWN` | `-1`
  `public static final int` | `BARCODE_UPCA` | `1`
  `public static final int` | `BARCODE_UPCA_2` | `39`
  `public static final int` | `BARCODE_UPCA_5` | `40`
  `public static final int` | `BARCODE_UPCE` | `41`
  `public static final int` | `BARCODE_UPCE_2` | `42`
  `public static final int` | `BARCODE_UPCE_5` | `43`

- com.datecs.biometric.TouchChip
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `IMAGE_COMPRESSION_NONE` | `0`
  `public static final int` | `IMAGE_COMPRESSION_WSQ` | `1`
  `public static final int` | `IMAGE_FORMAT_ANSI` | `0`
  `public static final int` | `IMAGE_FORMAT_ISO` | `1`
  `public static final int` | `IMAGE_FORMAT_RAW` | `2`
  `public static final int` | `IMAGE_SIZE_LARGE` | `1`
  `public static final int` | `IMAGE_SIZE_SMALL` | `0`
  `public static final int` | `TEMPLATE_FORMAT_ANSI` | `1`
  `public static final int` | `TEMPLATE_FORMAT_ISO_FMC_C` | `4`
  `public static final int` | `TEMPLATE_FORMAT_ISO_FMC_N` | `3`
  `public static final int` | `TEMPLATE_FORMAT_ISO_FMR` | `2`
  `public static final int` | `TEMPLATE_FORMAT_NATIVE` | `0`

- com.datecs.emsr.EMSR
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ENCRYPTION_TYPE_AES256` | `2`
  `public static final int` | `ENCRYPTION_TYPE_IDTECH` | `3`
  `public static final int` | `ENCRYPTION_TYPE_OLD_RSA` | `0`
  `public static final int` | `ENCRYPTION_TYPE_RSA` | `5`
  `public static final int` | `KEY_AES_AUTHENTICATION` | `0`
  `public static final int` | `KEY_AES_DATA_ENCRYPTION` | `1`
  `public static final int` | `KEY_AES_KEK` | `2`
  `public static final int` | `KEY_DUKPT_MASTER` | `32`
  `public static final int` | `KEY_NO_KEY` | `255`
  `public static final int` | `KEY_TMK_AES` | `16`
  `public static final int` | `MODE_READ_JIS` | `32`
  `public static final int` | `MODE_READ_PREFIX` | `128`
  `public static final int` | `MODE_READ_RAW` | `64`
  `public static final int` | `MODE_READ_TRACK1` | `1`
  `public static final int` | `MODE_READ_TRACK2` | `2`
  `public static final int` | `MODE_READ_TRACK3` | `4`
  `public static final int` | `STATUS_EMSR_BAD_ARRAY` | `16`
  `public static final int` | `STATUS_EMSR_BARCODE_MISHMASH` | `18`
  `public static final int` | `STATUS_EMSR_BARCODE_NO_READER` | `19`
  `public static final int` | `STATUS_EMSR_CARD_ERROR` | `3`
  `public static final int` | `STATUS_EMSR_HARD` | `23`
  `public static final int` | `STATUS_EMSR_INVALID_COMMAND` | `1`
  `public static final int` | `STATUS_EMSR_INVALID_LENGTH` | `20`
  `public static final int` | `STATUS_EMSR_INVALID_SIGNATURE` | `22`
  `public static final int` | `STATUS_EMSR_NO_BARCODE_READ` | `17`
  `public static final int` | `STATUS_EMSR_NO_DATA` | `6`
  `public static final int` | `STATUS_EMSR_NO_PERMISSION` | `2`
  `public static final int` | `STATUS_EMSR_NO_RESPONSE` | `5`
  `public static final int` | `STATUS_EMSR_SYNTAX_ERROR` | `4`
  `public static final int` | `STATUS_EMSR_TAMPERED` | `21`

- com.datecs.hub.Hub
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ERROR_COMMUNICATION` | `19`
  `public static final int` | `ERROR_INVALID_COMMAND` | `4`
  `public static final int` | `ERROR_INVALID_LENGTH` | `2`
  `public static final int` | `ERROR_NVRAM` | `20`
  `public static final int` | `ERROR_SLAVE` | `3`
  `public static final int` | `ERROR_TIMEOUT` | `5`
  `public static final int` | `EVENT_SLAVE_CONNECTED` | `1`
  `public static final int` | `EVENT_SLAVE_DATA_RECEIVED` | `3`
  `public static final int` | `EVENT_SLAVE_DISCONNECTED` | `2`
  `public static final int` | `EVENT_SLAVE_OVERCURRENT` | `4`
  `public static final int` | `SLAVE_STATE_DISCONNECTED` | `0`
  `public static final int` | `SLAVE_STATE_ERROR` | `3`
  `public static final int` | `SLAVE_STATE_READY` | `1`
  `public static final int` | `SLAVE_STATE_UNKNOWN` | `2`
  `public static final int` | `SLAVE_TYPE_RS232` | `2`
  `public static final int` | `SLAVE_TYPE_USB` | `1`

- com.datecs.linea.LineaPro
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `BARCODE_MODE_MOTION_DETECT` | `2`
  `public static final int` | `BARCODE_MODE_MULTI_SCAN` | `1`
  `public static final int` | `BARCODE_MODE_MULTI_SCAN_NO_DUPLICATE` | `4`
  `public static final int` | `BARCODE_MODE_SINGLE_SCAN` | `0`
  `public static final int` | `BARCODE_MODE_SINGLE_SCAN_ON_RELEASE` | `3`
  `public static final int` | `RFID_MODULE_CLRC663` | `1`
  `public static final int` | `RFID_MODULE_MURATA` | `0`

- com.datecs.linea.LineaProException
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ERROR_BUSY` | `9`
  `public static final int` | `ERROR_COM` | `13`
  `public static final int` | `ERROR_CONFIG` | `17`
  `public static final int` | `ERROR_CRYPT` | `15`
  `public static final int` | `ERROR_EMV` | `18`
  `public static final int` | `ERROR_FIRST_DATA` | `11`
  `public static final int` | `ERROR_FLASH` | `14`
  `public static final int` | `ERROR_GENERAL` | `1`
  `public static final int` | `ERROR_INVALID_AUTH` | `8`
  `public static final int` | `ERROR_INVALID_COMMAND` | `4`
  `public static final int` | `ERROR_INVALID_KEY` | `7`
  `public static final int` | `ERROR_INVALID_LENGTH` | `2`
  `public static final int` | `ERROR_INVALID_VALUE` | `3`
  `public static final int` | `ERROR_LAST_DATA` | `12`
  `public static final int` | `ERROR_NO` | `0`
  `public static final int` | `ERROR_NO_DATA` | `10`
  `public static final int` | `ERROR_NO_PERM` | `6`
  `public static final int` | `ERROR_OUT_OF_MEMORY` | `16`
  `public static final int` | `ERROR_TAMPERED` | `19`
  `public static final int` | `ERROR_TIMEOUT` | `5`

- com.datecs.printer.Printer
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ALIGN_CENTER` | `1`
  `public static final int` | `ALIGN_LEFT` | `0`
  `public static final int` | `ALIGN_RIGHT` | `2`
  `public static final int` | `BARCODE_CODABAR` | `71`
  `public static final int` | `BARCODE_CODE128` | `73`
  `public static final int` | `BARCODE_CODE128AUTO` | `75`
  `public static final int` | `BARCODE_CODE39` | `69`
  `public static final int` | `BARCODE_CODE93` | `72`
  `public static final int` | `BARCODE_EAN128` | `76`
  `public static final int` | `BARCODE_EAN13` | `67`
  `public static final int` | `BARCODE_EAN8` | `68`
  `public static final int` | `BARCODE_ITF` | `70`
  `public static final int` | `BARCODE_PDF417` | `74`
  `public static final int` | `BARCODE_UPCA` | `65`
  `public static final int` | `BARCODE_UPCE` | `66`
  `public static final int` | `FILL_BLACK` | `1`
  `public static final int` | `FILL_INVERTED` | `2`
  `public static final int` | `FILL_WHITE` | `0`
  `public static final int` | `HRI_ABOVE` | `1`
  `public static final int` | `HRI_BELOW` | `2`
  `public static final int` | `HRI_BOTH` | `3`
  `public static final int` | `HRI_NONE` | `0`
  `public static final int` | `PAGE_BOTTOM` | `1`
  `public static final int` | `PAGE_LEFT` | `0`
  `public static final int` | `PAGE_RIGHT` | `2`
  `public static final int` | `PAGE_TOP` | `3`
  `public static final int` | `SETTINGS_BLUETOOTH` | `5`

- com.datecs.printer.PrinterInformation
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `PRINTER_CMP10` | `0`
  `public static final int` | `PRINTER_DPP250` | `2`
  `public static final int` | `PRINTER_DPP350` | `1`
  `public static final int` | `PRINTER_DPP450` | `5`
  `public static final int` | `PRINTER_DPP500` | `8`
  `public static final int` | `PRINTER_EP300` | `7`
  `public static final int` | `PRINTER_EP55` | `4`
  `public static final int` | `PRINTER_EP60` | `6`
  `public static final int` | `PRINTER_PP60` | `3`
  `public static final int` | `PRINTER_UNKNOWN` | `-1`

- com.datecs.printer.ProtocolAdapter
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `CHANNEL_EMSR` | `15`
  `public static final int` | `CHANNEL_PRINTER` | `1`
  `public static final int` | `CHANNEL_RFID` | `13`
  `public static final int` | `CHANNEL_UNIVERSAL_READER` | `16`

- com.datecs.rfid.ContactlessCard
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `CARD_EPASSPORT` | `16`
  `public static final int` | `CARD_FELICA` | `11`
  `public static final int` | `CARD_ISO14443A` | `6`
  `public static final int` | `CARD_ISO14443B` | `10`
  `public static final int` | `CARD_ISO15693` | `8`
  `public static final int` | `CARD_MIFARE_CLASSIC_1K` | `2`
  `public static final int` | `CARD_MIFARE_CLASSIC_4K` | `3`
  `public static final int` | `CARD_MIFARE_DESFIRE` | `9`
  `public static final int` | `CARD_MIFARE_MINI` | `1`
  `public static final int` | `CARD_MIFARE_PLUS` | `7`
  `public static final int` | `CARD_MIFARE_ULTRALIGHT` | `4`
  `public static final int` | `CARD_MIFARE_ULTRALIGHT_C` | `5`
  `public static final int` | `CARD_PAYMENT` | `13`
  `public static final int` | `CARD_PICOPASS_14443B` | `15`
  `public static final int` | `CARD_PICOPASS_15693` | `14`
  `public static final int` | `CARD_ST_SRI` | `12`
  `public static final int` | `CARD_UNKNOWN` | `0`

- com.datecs.rfid.FeliCaCard
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `FELICA_SMARTTAG_BATTERY_LOW1` | `2`
  `public static final int` | `FELICA_SMARTTAG_BATTERY_LOW2` | `3`
  `public static final int` | `FELICA_SMARTTAG_BATTERY_NORMAL1` | `0`
  `public static final int` | `FELICA_SMARTTAG_BATTERY_NORMAL2` | `1`
  `public static final int` | `FELICA_SMARTTAG_DRAW_BLACK_BACKGROUND` | `1`
  `public static final int` | `FELICA_SMARTTAG_DRAW_KEEP_BACKGROUND` | `2`
  `public static final int` | `FELICA_SMARTTAG_DRAW_USE_LAYOUT` | `3`
  `public static final int` | `FELICA_SMARTTAG_DRAW_WHITE_BACKGROUND` | `0`

- com.datecs.rfid.RC663
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `CARD_SUPPORT_FELICA` | `4`
  `public static final int` | `CARD_SUPPORT_ISO15` | `32`
  `public static final int` | `CARD_SUPPORT_JEWEL` | `16`
  `public static final int` | `CARD_SUPPORT_NFC` | `8`
  `public static final int` | `CARD_SUPPORT_PICOPASS_ISO14` | `128`
  `public static final int` | `CARD_SUPPORT_PICOPASS_ISO15` | `256`
  `public static final int` | `CARD_SUPPORT_STSRI` | `64`
  `public static final int` | `CARD_SUPPORT_TYPE_A` | `1`
  `public static final int` | `CARD_SUPPORT_TYPE_B` | `2`
  `public static final int` | `CHANNEL_FELICA` | `4`
  `public static final int` | `CHANNEL_ISO1443A` | `1`
  `public static final int` | `CHANNEL_ISO1443B` | `2`
  `public static final int` | `CHANNEL_ISO15693` | `3`
  `public static final int` | `CHANNEL_MAIN` | `0`
  `public static final int` | `CHANNEL_STSRI` | `5`

- com.datecs.rfid.RFID
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `CARD_SUPPORT_FELICA` | `4`
  `public static final int` | `CARD_SUPPORT_ISO15` | `32`
  `public static final int` | `CARD_SUPPORT_JEWEL` | `16`
  `public static final int` | `CARD_SUPPORT_NFC` | `8`
  `public static final int` | `CARD_SUPPORT_STSRI` | `64`
  `public static final int` | `CARD_SUPPORT_TYPE_A` | `1`
  `public static final int` | `CARD_SUPPORT_TYPE_B` | `2`

- com.datecs.rfid.RFIDException
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ERROR_FAILED` | `-20`
  `public static final int` | `ERROR_MIFARE_EACCESS` | `-10013`
  `public static final int` | `ERROR_MIFARE_EAUTHENTICATION` | `-10010`
  `public static final int` | `ERROR_MIFARE_EBASE` | `-10000`
  `public static final int` | `ERROR_MIFARE_EBIT` | `-10012`
  `public static final int` | `ERROR_MIFARE_ECODE` | `-10011`
  `public static final int` | `ERROR_MIFARE_ECOLLISION` | `-10002`
  `public static final int` | `ERROR_MIFARE_ECRC` | `-10005`
  `public static final int` | `ERROR_MIFARE_EEEPROM` | `-10007`
  `public static final int` | `ERROR_MIFARE_EFIFO` | `-10006`
  `public static final int` | `ERROR_MIFARE_EFRAME` | `-10004`
  `public static final int` | `ERROR_MIFARE_EGENERIC` | `-10009`
  `public static final int` | `ERROR_MIFARE_EKEY` | `-10008`
  `public static final int` | `ERROR_MIFARE_EPARITY` | `-10003`
  `public static final int` | `ERROR_MIFARE_ETIMEOUT` | `-10001`
  `public static final int` | `ERROR_MIFARE_EVALUE` | `-10014`
  `public static final int` | `ERROR_TIMEOUT` | `-6`

- com.datecs.smartcard.AnswerToReset
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `PROTOCOL_T0` | `0`
  `public static final int` | `PROTOCOL_T1` | `1`

- com.datecs.universalreader.TouchEvent
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ACTION_DOWN` | `0`
  `public static final int` | `ACTION_UP` | `1`

- com.datecs.universalreader.UniversalReader
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `BUTTON_MODE_BARCODE` | `1`
  `public static final int` | `BUTTON_MODE_NONE` | `0`
  `public static final int` | `BUTTON_MODE_STATUS` | `2`
  `public static final int` | `CAPABILITY_BARCODE` | `4`
  `public static final int` | `CAPABILITY_BUTTON` | `64`
  `public static final int` | `CAPABILITY_DEBUG` | `1`
  `public static final int` | `CAPABILITY_EV15` | `1024`
  `public static final int` | `CAPABILITY_FIRMWARE` | `256`
  `public static final int` | `CAPABILITY_GSM` | `16`
  `public static final int` | `CAPABILITY_LCD2X16` | `128`
  `public static final int` | `CAPABILITY_MAGNETIC` | `512`
  `public static final int` | `CAPABILITY_MIFARE` | `32`
  `public static final int` | `CAPABILITY_SMARTCARD` | `2`
  `public static final int` | `CAPABILITY_TOUCHSCREEN` | `8`
  `public static final int` | `ERROR_0K` | `0`
  `public static final int` | `ERROR_BARCODE` | `16`
  `public static final int` | `ERROR_BARCODE_INVALID` | `18`
  `public static final int` | `ERROR_BARCODE_NODATA` | `17`
  `public static final int` | `ERROR_BARCODE_NOTPRESENT` | `19`
  `public static final int` | `ERROR_CARD` | `3`
  `public static final int` | `ERROR_INVALID` | `1`
  `public static final int` | `ERROR_MIFARE_ACCESS` | `-13`
  `public static final int` | `ERROR_MIFARE_AUTHENTICATION` | `-10`
  `public static final int` | `ERROR_MIFARE_BIT` | `-12`
  `public static final int` | `ERROR_MIFARE_CODE` | `-11`
  `public static final int` | `ERROR_MIFARE_COLLISION` | `-2`
  `public static final int` | `ERROR_MIFARE_CRC` | `-5`
  `public static final int` | `ERROR_MIFARE_EEPROM` | `-7`
  `public static final int` | `ERROR_MIFARE_FIFO` | `-6`
  `public static final int` | `ERROR_MIFARE_FRAME` | `-4`
  `public static final int` | `ERROR_MIFARE_GENERIC` | `-9`
  `public static final int` | `ERROR_MIFARE_KEY` | `-8`
  `public static final int` | `ERROR_MIFARE_PARITY` | `-3`
  `public static final int` | `ERROR_MIFARE_TIMEOUT` | `-1`
  `public static final int` | `ERROR_MIFARE_VALUE` | `-14`
  `public static final int` | `ERROR_NODATA` | `6`
  `public static final int` | `ERROR_NORESPONCE` | `5`
  `public static final int` | `ERROR_NOTPERMITTED` | `2`
  `public static final int` | `ERROR_SYNTAX` | `4`